{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXF-A"]
[]
[]
[]
[]
["","","","","","2AMXF40A2V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","550"]
["","","","Plotis","mm","765"]
["","","","Gylis","mm","285"]
["Svoris","Įrenginys","","","kg","36"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","aps. / min.","500"]
["","","Šildymas","Labai lėtai","aps. / min.","320"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-10"]
["","","","Maks.","°C DB","46"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","46"]
["","Šildymas","","Aukštas","dBA","48"]
["Šaltnešis","Tipas","","","","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.88"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.60"]
["Aušinimo medžiaga","GWP","","","","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 20m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15.0"]
["","","IU - IU","Maks.","m","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","30"]
["Standartiniai priedai","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Screw bag","","","","1"]
["El. tiekimas","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-230-240"]
["Pastabos","","","","","(1) - Vienai patalpai"]