{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","30","","","34"]
["","","Šildymas","Labai lėtai","m³/min.","32","","","34"]
["","","","Labai lėtai","cfm","1059","","","1200"]
["","","Šildymas","Labai lėtai","cfm","1130","","","1200"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550","550","550"]
["","","","Plotis","mm","765","765","765","765"]
["","","","Gylis","mm","285","285","285","285"]
["Svoris","Įrenginys","","","kg","36","36","36","41"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","rpm","760","500","500","890"]
["","","Šildymas","Labai lėtai","rpm","820","320","320","890"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10","-10","-10 (2)","-10"]
["","","","Maks.","°CDB","46","46","46 (2)","46"]
["","Šildymas","Aplinkos","Min.","° CWB","-15","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18","18"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","46","46"]
["","","","Nom.","dBA","48","","","46"]
["","Šildymas","","Aukštas","dBA","","48","48"]
["","","","Nom.","dBA","50","","","48"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.88","0.88","0.88","1.15"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["Aušinimo medžiaga","GWP","","","","675","675","675","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20","20","20 (1)","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 20m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15","15.0","15.0","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","30","30","30","30"]
["Standartiniai priedai","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50"]
["","Įtampa","","","V","220-240","220-230-240","220-230-240","220-240"]
["Pastabos","","","","","","(1) - Vienai patalpai"]
["","","","","","","","(1) - Vienai patalpai"]
["","","","","","","","(2) - Žr. specialų darbinio diapazono brėžinį"]
["Standartiniai priedai","Reducer assembly","","","","","","","1"]