{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M3V1B9","2MXM50M2V1B9"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550"]
["","","","Plotis","mm","765","765"]
["","","","Gylis","mm","285","285"]
["Svoris","Įrenginys","","","kg","41","41"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","Aps./min","500","500"]
["","","Šildymas","Labai lėtai","Aps./min","500","500"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","48","48"]
["","Šildymas","","Aukštas","dBA","50","50"]
["Šaltnešis","Tipas","","","","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.15","1.15"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.78","0.8"]
["Aušinimo medžiaga","GWP","","","","675","675.0"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 20m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","30","30"]
["Standartiniai priedai","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["El. tiekimas","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-230-240","220-230-240"]
["Pastabos","","","","","(1) - Vienai patalpai","(1) - Kiekvienas „D-AHU Professional“ gali būti sukurtas pagal jūsų poreikius. Pasirinkite savo AHU svetainėje tools.daikinapplied.eu"]