{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550","734"]
["","","","Plotis","mm","765","765","958"]
["","","","Gylis","mm","285","285","340"]
["Svoris","Įrenginys","","","kg","36","41","60"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","rpm","500","500","420"]
["","","Šildymas","Labai lėtai","rpm","320","500","420"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","46","48"]
["","","","Nom.","dBA","","","48"]
["","Šildymas","","Aukštas","dBA","48","50"]
["","","","Nom.","dBA","","","48.0"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.88","1.15","2"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.60","0.78","1.35"]
["Aušinimo medžiaga","GWP","","","","675","675","675.0"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20","20","25"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15.0","15.0","15.0"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","30","30","50"]
["Standartiniai priedai","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-230-240","220-230-240","220-240"]
["Pastabos","","","","","(1) - Vienai patalpai","(1) - Vienai patalpai","(1) - Vienai patalpai"]
["Standartiniai priedai","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]