{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B2","2MXS50H3V1B","2MXS50H2V1B"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","48","48","","50","50"]
["","Aušinimas","","Nom.","dBA","47","47","","48","48"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","1","","1","1"]
["","Sraigto maišas","","","","1","1","","1","1"]
["","Drenavimo čiaupas","","","","1","1","","1","1"]
["Šaltnešis","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Įkrova","","","kg","1.20","1.20","","1.60","1.60"]
["","Tipas","","","","R-410A","R-410A","","R-410A","R-410A"]
["Piping connections","Lygio skirtumas","IU - IU","Maks.","m","7.5","7.5","","7.5","7.5"]
["","","IU - OU","Maks.","m","15","15","","15","15"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 20m vamzdžiams)","","0,02 (ilgesniems kaip 20m vamzdžiams)","0,02 (ilgesniems kaip 20m vamzdžiams)"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","30","30","","30","30"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Matmenys","Vienetas","","Plotis","mm","765","765","","765","765"]
["","","","Gylis","mm","285","285","","285","285"]
["","","","Aukštis","mm","550","550","","550","550"]
["Svoris","Įrenginys","","","kg","38","38","","42","42"]
["Power supply","Fazė","","","","1~","1~","","1~","1~"]
["","Dažnis","","","Hz","50","50","","50","50"]
["","Įtampa","","","V","220-240","220-240","","220-240","220-240"]
["Pastabos","","","","","(1) - Yra floruotų šiltnamio efektą skatinančių dujų","(1) - Yra floruotų šiltnamio efektą skatinančių dujų","","(1) - Yra floruotų šiltnamio efektą skatinančių dujų","(1) - Yra floruotų šiltnamio efektą skatinančių dujų"]
["Matmenys","Įrenginys","","Aukštis","mm","","","550","","","550"]
["","","","Plotis","mm","","","765","","","765"]
["","","","Gylis","mm","","","285","","","285"]
["Svoris","Įrenginys","","","kg","","","38","","","42"]
["Kompresorius","Tipas","","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","","","10","","","10"]
["","","","Maks.","°CDB","","","46","","","46"]
["","Šildymas","Aplinkos","Min.","°CWB","","","-15","","","-15"]
["","","","Maks.","°CWB","","","15.5","","","15.5"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","","","47","","","48"]
["","Šildymas","","Nom.","dBA","","","48","","","50"]
["Šaltnešis","Tipas","","","","","","R-410A","","","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","","","1.20","","","1.60"]
["Šaltnešis","Užpildas","","","tCO2Eq","","","2.5","","","3.3"]
["Aušinimo medžiaga","GWP","","","","","","2087.5","","","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","","","20","","","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","","","0,02 (ilgesniems kaip 20m vamzdžiams)","","","0,02 (ilgesniems kaip 20m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","","","15","","","15"]
["","","IU - IU","Maks.","m","","","7.5","","","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","","","30","","","30"]
["Standartiniai priedai","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["El. tiekimas","Fazė","","","","","","1~","","","1~"]
["Maitinimas","Dažnis","","","Hz","","","50","","","50"]
["","Įtampa","","","V","","","220-240","","","220-240"]
["Standartiniai priedai","Reduktoriaus montažas","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]