{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","47"]
["","Aušinimas","","Nom.","dBA","46"]
["Standartiniai priedai","Įrengimo vadovas","","","","1"]
["","Sraigto maišas","","","","1"]
["","Drenavimo čiaupas","","","","1"]
["","Išleidimo dangtelis (1)","","","","6"]
["","Išleidimo dangtelis (2)","","","","3"]
["","Nulupama F tipo dujų etiketė","","","","1"]
["","Papildomo šaltnešio žymuo","","","","1"]
["Šaltnešis","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Įkrova","","","kg","1.8"]
["","Tipas","","","","R-32"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","rpm","420"]
["","","Šildymas","Labai lėtai","rpm","420"]
["Vamzdžių jungtys","Lygio skirtumas","IU - IU","Maks.","m","7.5"]
["","","IU - OU","Maks.","m","15"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","50"]
["Kompresorius","Type","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Matmenys","Įrenginys","","Plotis","mm","868"]
["","","","Gylis","mm","320"]
["","","","Aukštis","mm","734"]
["Svoris","Įrenginys","","","kg","57"]
["Power supply","Fazė","","","","1~"]
["","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-240"]
["Pastabos","","","","","(1) - Yra floruotų šiltnamio efektą skatinančių dujų"]
["","","","","","(2) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","(3) - Žr. atskirą elektros duomenų brėžinį"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","","24"]
["","","Šildymas","Labai lėtai","m³/min.","","24"]
["","","","Labai lėtai","cfm","","847"]
["","","Šildymas","Labai lėtai","cfm","","847"]
["Matmenys","Įrenginys","","Aukštis","mm","","734"]
["","","","Plotis","mm","","868"]
["","","","Gylis","mm","","320"]
["Svoris","Įrenginys","","","kg","","57"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","rpm","","420"]
["","","Šildymas","Labai lėtai","rpm","","420"]
["Kompresorius","Type","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","","-10"]
["","","","Maks.","°CDB","","46"]
["","Šildymas","Aplinkos","Min.","°CWB","","-15"]
["","","","Maks.","°CWB","","18"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","","46"]
["","Šildymas","","Nom.","dBA","","47"]
["Šaltnešis","Tipas","","","","","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","","1.80"]
["Šaltnešis","Užpildas","","","tCO2Eq","","1.2"]
["Aušinimo medžiaga","GWP","","","","","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","","25"]
["","Papildoma šaltnešio įkrova","","","kg/m","","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","","15"]
["","","IU - IU","Maks.","m","","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","","50"]
["Standartiniai priedai","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["El. tiekimas","Fazė","","","","","1~"]
["Maitinimas","Dažnis","","","Hz","","50"]
["","Įtampa","","","V","","220-240"]