{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-A8"]
[]
[]
[]
[]
["","","","","","3MXM40A2V1B8","3MXM52A2V1B8","3MXM68A2V1B8"]
["Matmenys","Įrenginys","","Aukštis","mm","734","734","734"]
["","","","Plotis","mm","974","974","974"]
["","","","Gylis","mm","408","408","408"]
["Svoris","Įrenginys","","","kg","57","57","62"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","50","50","50"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","46","46","48"]
["","Šildymas","","Nom.","dBA","47","47","48"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.80","1.80","2.00"]
["Šaltnešis","Užpildas","","","tCO2Eq","1.22","1.22","1.35"]
["Aušinimo medžiaga","GWP","","","","675","675","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","25 (1)","25 (1)","25 (1)"]
["","Papildoma šaltnešio įkrova","","","kg/m","002 (ilgesniems kaip 30m vamzdžiams)","002 (ilgesniems kaip 30m vamzdžiams)","002 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","50 (2)","50 (2)","50"]
["Standartiniai priedai","FTXJ42A2V1BS","","","","","FTXJ42A2V1BS"]
["","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]
["Pastabos","","","","","(1) - Vienai patalpai","(1) - Vienai patalpai","(1) - Vienai patalpai"]
["","","","","","(2) - Naudojant kartu su CVXM-A, FVXM-A – didžiausias vamzdžių ilgis 30 m.","(2) - Naudojant kartu su CVXM-A, FVXM-A – didžiausias vamzdžių ilgis 30 m.","(2) - Naudojant kartu su CVXM-A, FVXM-A – didžiausias vamzdžių ilgis 30 m."]
["","","","","","(3) - Žr. specialų darbinio diapazono brėžinį","(3) - Žr. specialų darbinio diapazono brėžinį","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","(4) - Žr. atskirą elektros duomenų brėžinį","(4) - Žr. atskirą elektros duomenų brėžinį","(4) - Žr. atskirą elektros duomenų brėžinį"]
["","","","","","(5) - Yra floruotų šiltnamio efektą skatinančių dujų","(5) - Yra floruotų šiltnamio efektą skatinančių dujų","(5) - Yra floruotų šiltnamio efektą skatinančių dujų"]
["Standartiniai priedai","FVXM25B2V1B","","","","","","FVXM25B2V1B"]