{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-M"]
[]
[]
[]
[]
["","","","","","3MXM40M2V1B","3MXM52M2V1B","3MXM68M2V1B"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","24","24","24.1"]
["","","Šildymas","Labai lėtai","m³/min.","24","24","24.1"]
["","","","Labai lėtai","cfm","847","847","851"]
["","","Šildymas","Labai lėtai","cfm","847","847","851"]
["Matmenys","Įrenginys","","Aukštis","mm","734","734","734"]
["","","","Plotis","mm","868","868","868"]
["","","","Gylis","mm","320","320","320"]
["Svoris","Įrenginys","","","kg","57","57","62"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","rpm","420","420"]
["","","Šildymas","Labai lėtai","rpm","420","420"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Šildymas","Aplinkos","Min.","° CWB","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","46","46","48"]
["","Šildymas","","Nom.","dBA","47","47","48"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.80","1.80","2.0"]
["Šaltnešis","Užpildas","","","tCO2Eq","1.2","1.2","1.4"]
["Aušinimo medžiaga","GWP","","","","675","675","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","25","25","25"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 30m vamzdžiams)","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","50","50"]
["Standartiniai priedai","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]
["Kompresorius","Tipas","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Standartiniai priedai","Drain cap","","","","","","9"]
["","Reducer assembly","","","","","","1"]