{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B2","4MXS80E3V3B","4MXS80E7V3B"]
["Matmenys","Įrenginys","","Aukštis","mm","770","770"]
["","","","Plotis","mm","900","900"]
["","","","Gylis","mm","320","320"]
["Svoris","Įrenginys","","","kg","72","72"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Vėsinimas","Aplinkos","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Šildymas","Aplinkos","Min.","° CWB","-15","-15"]
["","","","Maks.","° CWB","18","18"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","48","48"]
["","Šildymas","","Nom.","dBA","49","49"]
["Šaltnešis","Tipas","","","","R-410A","R-410A"]
["","Įkrova","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Vamzdžių jungtys","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 30m vamzdžiams)","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygių skirtumas","IU - OU","Maks.","m","15","15"]
["","","IU - IU","Maks.","m","7.5","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","70","70"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","1"]
["","Drenavimo čiaupas","","","","1","1"]
["","Reduktoriaus montažas","","","","1","1"]
["Power supply","Fazė","","","","1~","1~"]
["","Dažnis","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Pastabos","","","","","(1) - Aušinimas: temperatūra viduje 27 °CDB, 19.0 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m","(1) - Aušinimas: temperatūra viduje 27 °CDB, 19.0 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m"]
["","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m"]
["","","","","","(3) - Yra floruotų šiltnamio efektą skatinančių dujų","(3) - Yra floruotų šiltnamio efektą skatinančių dujų"]
["Matmenys","Įrenginys","","Aukštis","mm","","","770"]
["","","","Plotis","mm","","","900"]
["","","","Gylis","mm","","","320"]
["Svoris","Įrenginys","","","kg","","","72"]
["Kompresorius","Tipas","","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Šildymas","Aplinkos","Min.","° CWB","","","-15"]
["","","","Maks.","° CWB","","","15.5"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","","","48"]
["","Šildymas","","Nom.","dBA","","","49"]
["Šaltnešis","Tipas","","","","","","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","","","2.99"]
["Šaltnešis","Užpildas","","","tCO2Eq","","","6.2"]
["Aušinimo medžiaga","GWP","","","","","","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","","","25"]
["","Papildoma šaltnešio įkrova","","","kg/m","","","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","","","15"]
["","","IU - IU","Maks.","m","","","7.5"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","","","70"]
["Standartiniai priedai","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["El. tiekimas","Fazė","","","","","","1~"]
["Maitinimas","Dažnis","","","Hz","","","50"]
["","Įtampa","","","V","","","230"]