{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MWXM-A9"]
[]
[]
[]
[]
["","","","","","5MWXM68A2V1B9","5MWXM90A2V1B9"]
["Matmenys","Įrenginys","","Aukštis","mm","734","734"]
["","","","Plotis","mm","1,040","1,040"]
["","","","Gylis","mm","408","408"]
["Svoris","Įrenginys","","","kg","69","73"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-10","-10"]
["","","","Maks.","°C DB","46","46"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","48","52"]
["","Šildymas","","Nom.","dBA","49","53"]
["Šaltnešis","Tipas","","","","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","2","2.4"]
["Šaltnešis","Užpildas","","","tCO2Eq","1.35","1.62"]
["Aušinimo medžiaga","GWP","","","","675","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","25 (2)","25 (3)"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 30m vamzdžiams)","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15 (3)","15"]
["","","IU - IU","Maks.","m","7.5 (3)","7.5 (3)"]
["","Bendras vamzdžių ilgis","Sistema","Faktiškai","m","60","75"]
["Standartiniai priedai","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","2","2"]
["El. tiekimas","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-440","220-240"]
["Pastabos","","","","","(1) - Žr. specialų darbinio diapazono brėžinį","(1) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","(2) - Vienai patalpai","(2) - Vienai patalpai"]
["","","","","","(3) - Vienai patalpai (derinant su FBA71/100/125 ir EKHWET bei CKHWS, žiūrėkite montavimo vadove)","(3) - Vienai patalpai (derinant su FBA71/100/125 ir EKHWET bei CKHWS, žiūrėkite montavimo vadove)"]
["","","","","","(4) - Yra floruotų šiltnamio efektą skatinančių dujų","(4) - Yra floruotų šiltnamio efektą skatinančių dujų"]