{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1 UK"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B UK","ABQ125CV1 / AZQS125B7Y1B UK","ABQ140CV1 / AZQS140B7Y1B UK"]
["Aušinimo galingumas","Nom.","","kW","9.5","12.1","13.0"]
["Patalpos vėsinimas","SEER","","","4.65"]
["","Metinės energijos sąnaudos","","kWh/a","716"]
["","Vėsinimas","Pdesign","kW","9.50"]
["","Energijos efektyvumo klasė","","","B"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","6.78"]
["","SCOP/A","","","3.80"]
["","Energijos efektyvumo klasė","","","A"]
["","Metinės energijos sąnaudos","","kWh/a","2,498"]
["Vardinis našumas","Annual energy consumption","","kWh","1,810","2,153","2,159"]
["","EER","","","2.62","2.81","3.01"]
["","COP","","","3.42","3.41","3.41"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","D","C"]
["","","Šildymas","","B","B"]
["Šildymo galingumas","Nom.","","kW","10.8","13.5","15.5"]
["Pastabos","","","","(1) - Metinės energijos sąnaudos pagal energijos žymėjimo direktyvą 2002/31/EB","(1) - Metinės energijos sąnaudos pagal energijos žymėjimo direktyvą 2002/31/EB","(1) - Metinės energijos sąnaudos pagal energijos žymėjimo direktyvą 2002/31/EB"]
["","","","","(2) - SEER ir SCOP pagal EN 14825","(2) - SEER ir SCOP pagal EN 14825","(2) - SEER ir SCOP pagal EN 14825"]
["","","","","(3) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(3) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","(3) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]