{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Tylus veikimas","dBA","","36","","41"]
["","","","Žemas","dBA","","38","","43"]
["","Aušinimas","","Tylus veikimas","dBA","","36","","41"]
["","","","Žemas","dBA","","38","","43"]
["","","","Aukštas","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standartiniai priedai","Įrengimo vadovas","","","","","Įrengimo vadovas","","Įrengimo vadovas"]
["","Eksploatavimo vadovas","","","","","Eksploatavimo vadovas","","Eksploatavimo vadovas"]
["","Varžtai","","","","","Varžtai","","Varžtai"]
["","Poveržlė","","","","","Poveržlė","","Poveržlė"]
["","Belaidis nuotolinis valdymas","","","","","Belaidis nuotolinis valdymas","","Belaidis nuotolinis valdymas"]
["","Gaubto užrakinamos grotelės","","","","","Gaubto užrakinamos grotelės","","Gaubto užrakinamos grotelės"]
["","Baterija","","","","","Baterija","","Baterija"]
["Kontrolės sistemos","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Vamzdžių jungtys","Skystis","","OD","mm","","9.52","","9.52"]
["","Dujos","","OD","mm","","15.88","","15.88"]
["","Drain","","","","","19.05","","19.05"]
["Power input","Aušinimas","","Nom.","kW","","0.094","","0.137"]
["","Šildymas","","Nom.","kW","","0.094","","0.137"]
["Sound power level","Cooling","","","dBA","","56","","60"]
["","Heating","","","dBA","","56","","60"]
["Matmenys","Įrenginys","","Plotis","mm","","820","","820"]
["","","","Gylis","mm","","820","","820"]
["","","","Aukštis","mm","","300","","300"]
["Korpusas","Medžiaga","","","","","Galvanizuotas plienas","","Galvanizuotas plienas"]
["Svoris","Įrenginys","","","kg","","39","","39"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","","29.2","","34.0"]
["","","","Mažas","m³/min.","","21.0","","26.3"]
["","","","Nom.","m³/min.","","24.4","","29.2"]
["","","Aušinimas","Mažas","m³/min.","","21.0","","26.3"]
["","","","Nom.","m³/min.","","24.4","","29.2"]
["","","","Didelis","m³/min.","","29.2","","34.0"]
["","","","Tylus veikimas","m³/min.","","17.6","","22.1"]
["","","Aušinimas","Tylus veikimas","m³/min.","","17.6","","22.1"]
["Dekoratyvinis skydelis","Svoris","","","kg","","4","","4"]
["","Matmenys","","Aukštis","mm","","82","","82"]
["","","","Gylis","mm","","990","","990"]
["","","","Plotis","mm","","990","","990"]
["","Spalva","","","","","Balta spalva","","Balta spalva"]
["Power supply","Phase","","","","","1~","","1~"]
["","Name","","","","","V1","","V1"]
["","Dažnis","","","Hz","","50","","50"]
["","Įtampa","","","V","","220-240","","220-240"]
["Ventiliatorius","Oro debitas","Šildymas","Tylus veikimas","m³/min.","15","","22.1"]
["Tiekiama galia","Šildymas","","Nom.","kW","0.067","","0.137"]
["","Aušinimas","","Nom.","kW","0.067","","0.137"]
["Ventiliatorius","Oro debitas","Aušinimas","Tylus veikimas","m³/min.","15","","22.1"]
["Korpusas","Medžiaga","","","","Galvanizuotas plienas","","Galvanizuotas plienas"]
["Matmenys","Įrenginys","","Aukštis","mm","265","","300"]
["","","","Plotis","mm","820","","820"]
["","","","Gylis","mm","820","","820"]
["Svoris","Įrenginys","","","kg","31","","39"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","24.4","","34"]
["","","","Nom.","m³/min.","20.5","","29.2"]
["","","","Mažas","m³/min.","17.6","","26.3"]
["","","Šildymas","Didelis","m³/min.","24.4","","34"]
["","","","Nom.","m³/min.","20.5","","29.2"]
["","","","Mažas","m³/min.","17.6","","26.3"]
["Garso galingumo lygis","Vėsinimas","","","dBA","54","","60"]
["","Šildymas","","","dBA","54","","60"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Žemas","dBA","35","","43"]
["","","","Tylus veikimas","dBA","32","","41"]
["","Šildymas","","Aukštas","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Žemas","dBA","35","","43"]
["","","","Tylus veikimas","dBA","32","","41"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52","","9.52"]
["","Dujos","","Iš. diam.","mm","15.88","","15.88"]
["","Drenažas","","","","19.05","","19.05"]
["Dekoratyvinis skydelis","Matmenys","","Aukštis","mm","82","","82"]
["","","","Plotis","mm","990","","990"]
["","","","Gylis","mm","990","","990"]
["","Svoris","","","kg","4","","4"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARCWLA","","ARCWLA"]
["","Laidinis nuotolinio valdymo pultelis","","","","ARCWB","","ARCWB"]
["Standartiniai priedai","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["El. tiekimas","Fazė","","","","1~","","1~"]
["Maitinimas","Dažnis","","","Hz","50","","50"]
["","Įtampa","","","V","220-240","","220-240"]