{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","AHQ125CV1 / AZQS125B7Y1B","AHQ140CV1 / AZQS140B7Y1B","AHQ100CV1 / AZQS100B7Y1B"]
["Aušinimo galingumas","Nom.","","kW","12.1 (1)","13.0 (1)","9.5"]
["Erdvės vėsinimas","SEER","","","5.14","5.77","4.60"]
["","Metinės energijos sąnaudos","","kWh/m.","1,412","1,353","723"]
["","Vėsinimas","Pdesign","kW","12.1","13.0","9.50"]
["","Energijos efektyvumo klasė","","","","","B"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","7.99","11.97","7.60"]
["","SCOP/A","","","3.78","3.99","3.80"]
["","Energijos efektyvumo klasė","","","","","A"]
["","Metinės energijos sąnaudos","","kWh/m.","2,964","4,199","2,800"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","","","1,810"]
["","EER","","","2.22 (3)","2.63 (3)","2.62"]
["","COP","","","","","3.41"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","D"]
["","","Šildymas","","","","B"]
["Šildymo galingumas","Nom.","","kW","13.5 (2)","15.5 (2)","10.8"]
["Pastabos","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 7,5 m; aukščių skirtumas: 0 m","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]
["","","","","(3) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","(3) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]