{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Tiekiama galia","Šildymas","","Nom.","kW","0.106","0.149"]
["","Aušinimas","","Nom.","kW","0.106","0.149"]
["Ventiliatorius","Išorinis statinis slėgis","","Aukštas","Pa","0","0","0","0"]
["","","","Žemas","Pa","0","0","0","0"]
["Aušinimo galingumas","Bendras galingumas","","Nom.","kW","","","12.10","13.00"]
["Šildymo galia","Bendras pajėgumas","","Nom.","kW","","","13.5","15.5"]
["Korpusas","Spalva","","","","Balta","Balta","Balta","Balta"]
["","Medžiaga","","","","Galvanizuotas plienas","Galvanizuotas plienas"]
["Matmenys","Įrenginys","","Aukštis","mm","260","260","260","285"]
["","","","Plotis","mm","1320","1538","1790","1900"]
["","","","Gylis","mm","634","634","634","680"]
["Svoris","Įrenginys","","","kg","38","45","65","70"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min.","21.3","27.8","31","39"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","","31","39"]
["","","","Mažas","m³/min.","18.9","24.8","27.2","28.3"]
["","","Šildymas","Didelis","m³/min.","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min.","21.3","27.8","30.6","39.1"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","","30.6","39.1"]
["","","Šildymas","Mažas","m³/min.","18.9","24.8","27.2","28.3"]
["","Išorinis statinis slėgis","","Nom.","Pa","0","0","0","0"]
["Garso galingumo lygis","Vėsinimas","","","dBA","59","64","65","71"]
["","Šildymas","","","dBA","62","64","65","71"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["","Vėsinimas","","Vidutinis","dBA","","","50","53"]
["","","","Žemas","dBA","46","46","49","46"]
["","Šildymas","","Aukštas","dBA","49","52","52","56"]
["","","","Vidutinis","dBA","","","50","53"]
["","","","Nom.","dBA","48","47"]
["","","","Žemas","dBA","46","46","49","46"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52","9.52","9.52","9.52"]
["","Dujos","","Iš. diam.","mm","15.88","15.88","15.9","15.9"]
["","Drenažas","","","","19.05","19.05"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Laidinis nuotolinio valdymo pultelis","","","","ARCWB","ARCWB"]
["Standartiniai priedai","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Išleidimo vamzdis","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["El. tiekimas","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]