{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B","ARXM35R5V1B","ARXM50R2V1B","ARXM50R5V1B","ARXM60R5V1B","ARXM60R2V1B","ARXM71R5V1B","ARXM71R2V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550","734","734","734","734","734","734"]
["","","","Plotis","mm","765","765","954","954","954","954","954","954"]
["","","","Gylis","mm","285","285","401","401","401","401","401","401"]
["Svoris","Įrenginys","","","kg","32","32","49.0","49.0","49.0","49.0","49.0","49.0"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-10","-10","-10","-10 (4) (5), -10 (4) (5)","-10","-10","-10","-10"]
["","","","Maks.","°C DB","50, 46","50, 46","50, 46","50 (4), 46 (5)","46","46","46","46"]
["","Šildymas","Aplinkos","Min.","° CWB","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","46","49","48.0","48.0","48.0","48.0","52.0","52.0"]
["","Šildymas","","Nom.","dBA","47","49","49.0","49.0","49.0","49.0","52.0","52.0"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.76","0.76","1.15","1.15","1.15","1.15","1.15","1.15"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.52","0.52","0.780","0.780","0.780","0.780","0.780","0.780"]
["Aušinimo medžiaga","GWP","","","","675","675","675.0","675.0","675.0","675.0","675.0","675.0"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20","20","30","30","30","30","30","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,035 (ilgesniems kaip 10 m vamzdžiams)","0,035 (ilgesniems kaip 10 m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15","15","20.0","20.0","20.0","20.0","20.0","20.0"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50","50","50"]
["Standartiniai priedai","Drain cap","","","","","","3","3","3","3","3","3"]
["Pastabos","","","","","","","","(1) - Galima taikyti tik kartu su CTXM*N2V1B, ATXM*N2V1B, FTXM*N2V1B"]
["","","","","","","","","(2) - Galima naudoti tik su CTXM*M2V1B, ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9,FBA*A2VEB9, FHA*AVEB9, FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB·"]