{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","","49.0"]
["","Aušinimas","","Nom.","dBA","","49.0"]
["Standartiniai priedai","Drenavimo čiaupas","","","","","1"]
["","Įrengimo vadovas","","","","","1"]
["","Užpildymo šaltnešiu etiketė","","","","","1"]
["","Etiketės apie floruotas šiltnamio efektą skatinančias dujas įvairiomis kalbomis","","","","","1"]
["","Bendrosios saugos priemonės","","","","","1"]
["Šaltnešis","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Įkrova","","","kg","","0.76"]
["","Type","","","","","R-32"]
["Veikimo diapazonas","Vėsinimas","Aplinkos","Maks.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Vamzdžių jungtys","Lygių skirtumas","IU - OU","Maks.","m","","15"]
["","Papildoma šaltnešio įkrova","","","kg/m","","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["Compressor","Tipas","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Matmenys","Vienetas","","Plotis","mm","","840"]
["","","","Gylis","mm","","350"]
["","","","Aukštis","mm","","552"]
["Svoris","Vienetas","","","kg","","32"]
["Power supply","Fazė","","","","","1~"]
["","Dažnis","","","Hz","","50"]
["","Įtampa","","","V","","220-240"]
["Pastabos","","","","","(1) - Galima tik kartu su ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Yra floruotų šiltnamio efektą skatinančių dujų"]
["","","","","","(2) - Galima tik kartu su ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","","(3) - Žr. atskirą elektros duomenų brėžinį"]
["","","","","","","(4) - Galima tik kartu su ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Galima tik kartu su ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","552"]
["","","","Plotis","mm","840"]
["","","","Gylis","mm","350"]
["Svoris","Įrenginys","","","kg","32"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (4), 46 (5)"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","46.0"]
["","Šildymas","","Nom.","dBA","47.0"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.76"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.52"]
["Aušinimo medžiaga","GWP","","","","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15"]
["Standartiniai priedai","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Maitinimas","Dažnis","","","Hz","50"]