{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","","48"]
["","","","Žemas","dBA","","45"]
["Standartiniai priedai","1","","","","","550"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","","2.5"]
["","Tipas","","","","","1.2"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","","30.1"]
["","","","Labai lėtai","cfm","","1,063"]
["Ventiliatoriaus variklis","Greitis","Aušinimas","Labai lėtai","aps. / min.","","740"]
["","","Šildymas","Labai lėtai","aps. / min.","","-15"]
["Veikimo diapazonas","Heating","Aplinkos","Min.","°CWB","","20"]
["","","","Maks.","°CWB","","10"]
["Garso slėgio lygis","Aušinimas","","Žemas","dBA","","44"]
["","","","Aukštas","dBA","","48"]
["Kompresorius","Type","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Matmenys","Vienetas","","Plotis","mm","","285"]
["","","","Gylis","mm","","612"]
["","","","Aukštis","mm","","765"]
["Svoris","Įrenginys","","","kg","","34"]
["Ventiliatorius","Oro debitas","Šildymas","Labai lėtai","cfm","","904"]
["","","","Labai lėtai","m³/min.","","25.6"]
["Power supply","Fazė","","","","","1~"]
["","Dažnis","","","Hz","","50"]
["","Įtampa","","","V","","220-240"]
["Pastabos","","","","","(1) - 220 V","(1) - Yra floruotų šiltnamio efektą skatinančių dujų"]
["","","","","","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 230 V"]
["","","","","","","(4) - 240 V"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","30.1"]
["","","Šildymas","Labai lėtai","m³/min.","25.6"]
["","","","Labai lėtai","cfm","1063"]
["","","Šildymas","Labai lėtai","cfm","904"]
["Matmenys","Įrenginys","","Aukštis","mm","550"]
["","","","Plotis","mm","765"]
["","","","Gylis","mm","285"]
["Svoris","Įrenginys","","","kg","34"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","aps. / min.","780"]
["","","Šildymas","Labai lėtai","aps. / min.","740"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","10"]
["","","","Maks.","°C DB","46"]
["","Šildymas","Aplinkos","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","46"]
["","Šildymas","","Aukštas","dBA","47"]
["","","","Žemas","dBA","44"]
["Šaltnešis","Tipas","","","","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.0"]
["Šaltnešis","Užpildas","","","tCO2Eq","2.1"]
["Aušinimo medžiaga","GWP","","","","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15"]
["Standartiniai priedai","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["El. tiekimas","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-240"]