{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","","","","","","43"]
["","","","Vidutinis","dBA","","","","","","35"]
["","","","Tylus veikimas","dBA","","","","","","26"]
["","","","Žemas","dBA","","","","","","29"]
["","Aušinimas","","Vidutinis","dBA","","","","","","34"]
["","","","Tylus veikimas","dBA","","","","","","20"]
["","","","Žemas","dBA","","","","","","27"]
["","","","Aukštas","dBA","","","","","","43"]
["Standartiniai priedai","Įrengimo vadovas","","","","","","","","","1"]
["","Eksploatavimo vadovas","","","","","","","","","1"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","","","","","","","1"]
["","AA sausosios baterijos","","","","","","","","","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","","","","","","1"]
["","Pritvirtinimo plokštė","","","","","","","","","1"]
["","Titano apatito fotokatalizatoriaus oro gryninimo filtras","","","","","","","","","2"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","","","","","","2"]
["Kontrolės sistemos","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Vamzdžių jungtys","Skystis","","OD","mm","","","","","","6.35"]
["","Dujos","","Iš. diam.","mm","","","","","","9.50"]
["","Drenažo vamzdis","","","","","","","","","18"]
["Tiekiamas galingumas","Aušinimas","","Nom.","kW","","","","","","0.024"]
["","Šildymas","","Nom.","kW","","","","","","0.029"]
["Sound power level","Vėsinimas","","","dBA","","","","","","58"]
["","Šildymas","","","dBA","","","","","","58"]
["Matmenys","Įrenginys","","Plotis","mm","","","","","","770"]
["","","","Gylis","mm","","","","","","225"]
["","","","Aukštis","mm","","","","","","286"]
["Korpusas","Spalva","","","","","","","","","Balta spalva"]
["Svoris","Įrenginys","","","kg","","","","","","9.0"]
["Power supply","Fazė","","","","","","","","","1~"]
["","Dažnis","","","Hz","","","","","","50"]
["","Pavadinimas","","","","","","","","","V1"]
["","Įtampa","","","V","","","","","","220-240"]
["Pastabos","","","","","","","","","","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Šildymas","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Korpusas","Spalva","","","","Balta","Balta","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","286","286","286","286","286"]
["","","","Plotis","mm","770","770","770","770","770"]
["","","","Gylis","mm","225","225","225","225","225"]
["Svoris","Įrenginys","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","9.9","9.9","10.4","10.4","11.8"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7.8","7.8","8","8","8.2"]
["","","","Mažas","m³/min.","5.8","5.8","6.1","6.1","6.3"]
["","","","Tylus veikimas","m³/min.","4.8","4.8","4.8","4.8","4.9"]
["","","Šildymas","Didelis","m³/min.","10.9","10.9","11.1","11.1","12.8"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.5","8.5","8.5","8.5","8.5"]
["","","Šildymas","Mažas","m³/min.","6.4","6.4","6.7","6.7","6.9"]
["","","","Tylus veikimas","m³/min.","5.2","5.2","5.2","5.2","5.2"]
["Garso galingumo lygis","Vėsinimas","","","dBA","55","55","55","55","58"]
["","Šildymas","","","dBA","55","55","55","55","58"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","39","39","40","40","43"]
["","Vėsinimas","","Vidutinis","dBA","33","33","33","33","34"]
["","","","Žemas","dBA","25","25","26","26","27"]
["","","","Tylus veikimas","dBA","20","20","20","20","20"]
["","Šildymas","","Aukštas","dBA","39","39","40","40","43"]
["","","","Vidutinis","dBA","34","34","34","34","35"]
["","","","Žemas","dBA","28","28","28","28","29"]
["","","","Tylus veikimas","dBA","23","23","23","23","26"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5","9.5","9.5","9.5"]
["","Drenažas","","","","18","18","18","18","18"]
["Kontrolės sistemos","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["El. tiekimas","Pavadinimas","","","","V1","V1","V1","V1","V1"]
["","Fazė","","","","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standartiniai priedai","AAA dry-cell batteries","","","","","2","","2","2"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","","","ARC480A11","ARC480A11"]
["Standartiniai priedai","Titanium apatite photocatalytic air purification filter","","","","","","2"]