{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A / 3AMXF-A9"]
[]
[]
[]
[]
["","","","","ATXF25A5V1B / ATXF25A5V1B / ATXF25A5V1B / 3AMXF52A2V1B9"]
["Aušinimo galingumas","Min.","","kW","1.8"]
["","Nom.","","kW","5.2"]
["","Maks.","","kW","7"]
["Šildymo galingumas","Min.","","kW","1.3"]
["","Nom.","","kW","6.8"]
["","Maks.","","kW","8"]
["Nominalus efektyvumas","EER","","","4.05"]
["","COP","","","3.88"]
["","Metinis energijos sunaudojimas","","kWh","642"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A"]
["","","Šildymas","","A"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A++"]
["","Vėsinimas","Pdesign","kW","5.2"]
["","SEER","","","7.2"]
["","Metinės energijos sąnaudos","","kWh/m.","253"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A+"]
["","Pajėgumas","Pdesign","kW","5"]
["","SCOP/A","","","4.01"]
["","Pdh Šildymo pajėgumas esant –10°","","kW","3.74"]
["","Metinės energijos sąnaudos","","kWh/m.","1744"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D"]