{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","40","42","44","45"]
["","","","Vidutinis","dBA","34","38","40","41"]
["","","","Tylus veikimas","dBA","21","30","32","33"]
["","","","Žemas","dBA","28","33","35","36"]
["","Aušinimas","","Medium","dBA","33","39","41","42"]
["","","","Tylus veikimas","dBA","20","31","33","34"]
["","","","Žemas","dBA","26","34","36","37"]
["","","","Aukštas","dBA","40","43","45","46"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","1","1","1"]
["","Eksploatavimo vadovas","","","","1","1","1","1"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","","1","1","1","1"]
["","AAA sausosios baterijos","","","","2","2","2","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","1","1","1","1"]
["","Pritvirtinimo plokštė","","","","1","1","1","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","2","2","2","2"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.50","12.7","12.7","12.7"]
["","Drain","","","","18","18","18","18"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.019","0.029","0.032","0.032"]
["","Šildymas","","Nom.","kW","0.020","0.032","0.035","0.035"]
["Triukšmingumo lygis","Vėsinimas","","","dBA","55","59","60","62"]
["","Šildymas","","","dBA","55","61","62","62"]
["Matmenys","Įrenginys","","Plotis","mm","770","990","990","990"]
["","","","Gylis","mm","225","263","263","263"]
["","","","Aukštis","mm","286","295","295","295"]
["Korpusas","Spalva","","","","Balta spalva","Balta spalva","Balta spalva","Balta spalva"]
["Svoris","Įrenginys","","","kg","8.50","13.5","13.5","13.5"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","10.3","17.3","17.9","17.9"]
["","","","Mažas","m³/min.","6.7","12.2","12.8","12.8"]
["","","","Vidutinis","m³/min.","8.6","14.8","15.8","15.8"]
["","","","Tylus veikimas","m³/min.","5.3","10.7","11.3","11.3"]
["","","Vėsinimas","Mažas","m³/min.","6.1","11.9","12.2","12.2"]
["","","","Vidutinis","m³/min.","8.1","14.4","14.8","14.8"]
["","","","Didelis","m³/min.","10.1","16.8","17.3","17.3"]
["","","","Tylus veikimas","m³/min.","4.4","10.5","10.7","10.7"]
["Power supply","Fazė","","","","1~","1~","1~","1~"]
["","Dažnis","","","Hz","50","50","50","50"]
["","Pavadinimas","","","","","V1","V1","V1"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","","","","0.019","0.032"]
["","Šildymas","","Nom.","kW","","","","","0.02","0.032"]
["Korpusas","Spalva","","","","","","","","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","","","","","286","286"]
["","","","Plotis","mm","","","","","770","770"]
["","","","Gylis","mm","","","","","225","225"]
["Svoris","Įrenginys","","","kg","","","","","8.5","9"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","","","","10.1","11.5"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","","","","8.1","8.3"]
["","","","Mažas","m³/min.","","","","","6.1","6.3"]
["","","","Tylus veikimas","m³/min.","","","","","4.4","4.5"]
["","","Šildymas","Didelis","m³/min.","","","","","10.3","11.5"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","","","","8.6","9"]
["","","Šildymas","Mažas","m³/min.","","","","","6.7","7"]
["","","","Tylus veikimas","m³/min.","","","","","5.3","5.3"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","","","","55","58"]
["","Šildymas","","","dBA","","","","","55","58"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","","","","40","43"]
["","Vėsinimas","","Vidutinis","dBA","","","","","33","34"]
["","","","Žemas","dBA","","","","","26","27"]
["","","","Tylus veikimas","dBA","","","","","20","20"]
["","Šildymas","","Aukštas","dBA","","","","","40","40"]
["","","","Vidutinis","dBA","","","","","34","35"]
["","","","Žemas","dBA","","","","","28","29"]
["","","","Tylus veikimas","dBA","","","","","21","21"]
["Vamzdžių jungtys","Skystis","","OD","mm","","","","","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","","","","","9.5","9.5"]
["","Drenažas","","","","","","","","18","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","","","","","ARC470A1","ARC470A1"]
["","Laidinis nuotolinio valdymo pultelis","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standartiniai priedai","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["El. tiekimas","Fazė","","","","","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","","","","","50","50"]
["","Įtampa","","","V","","","","","220-240","220-240"]