{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-G"]
[]
[]
[]
[]
["","","","","","ATXF25G5V1B","ATXF35G5V1B"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.023","0.029"]
["","Šildymas","","Nom.","kW","0.023","0.023"]
["Korpusas","Spalva","","","","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","286","286"]
["","","","Plotis","mm","770","770"]
["","","","Gylis","mm","225","225"]
["Svoris","Įrenginys","","","kg","8.5","9"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","9.8","10.9"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","8","7"]
["","","","Mažas","m³/min.","6","5.7"]
["","","","Tylus veikimas","m³/min.","4.3","4.6"]
["","","Šildymas","Didelis","m³/min.","10.4","9.3"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.4","7.5"]
["","","Šildymas","Mažas","m³/min.","6.4","6"]
["","","","Tylus veikimas","m³/min.","5.3","5.2"]
["Garso galingumo lygis","Vėsinimas","","","dBA","54","54"]
["","Šildymas","","","dBA","55","56"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","40","56"]
["","Vėsinimas","","Vidutinis","dBA","33"]
["","","","Žemas","dBA","26"]
["","","","Tylus veikimas","dBA","20"]
["","Šildymas","","Aukštas","dBA","40","40"]
["","","","Vidutinis","dBA","34","35"]
["","","","Žemas","dBA","28","29"]
["","","","Tylus veikimas","dBA","21","21"]
["Vamzdžių jungtys","Skystis","","OD","mm","6","6"]
["","Dujos","","Iš. diam.","mm","9.5","9.5"]
["","Drenažas","","","","18","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARC480A93","ARC480A93"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["El. tiekimas","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-440","220-440"]
["Pastabos","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB; ekvivalentinis vamzdyno ilgis: 5 m; aukščių skirtumas: 0 m"]
["","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m (horizontaliai)","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m (horizontaliai)"]
["","","","","","(3) - Žr. atskirą elektros duomenų brėžinį","(3) - Žr. atskirą elektros duomenų brėžinį"]