{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","39"]
["","","","Vidutinis","dBA","34"]
["","","","Tylus veikimas","dBA","20"]
["","","","Žemas","dBA","26"]
["","Aušinimas","","Vidutinis","dBA","33"]
["","","","Tylus veikimas","dBA","19"]
["","","","Žemas","dBA","25"]
["","","","Aukštas","dBA","41"]
["Standartiniai priedai","Įrengimo vadovas","","","","1"]
["","Eksploatavimo vadovas","","","","1"]
["","Belaidis nuotolinis valdymas","","","","1"]
["","AAA sausosios baterijos","","","","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","1"]
["","Pritvirtinimo plokštė","","","","1"]
["","Dezodoruojantis filtras iš titano ir apatito","","","","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","2"]
["","WLAN adapterio rinkinys","","","","1"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35"]
["","Dujos","","Iš. diam.","mm","9.50"]
["","Drenažo vamzdis","","","","18"]
["Power input","Aušinimas","","Nom.","kW","0.029"]
["","Šildymas","","Nom.","kW","0.023"]
["Sound power level","Vėsinimas","","","dBA","58"]
["","Šildymas","","","dBA","55"]
["Matmenys","Įrenginys","","Plotis","mm","778"]
["","","","Gylis","mm","272"]
["","","","Aukštis","mm","295"]
["Korpusas","Spalva","","","","Balta spalva"]
["Svoris","Įrenginys","","","kg","10.0"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","9.3"]
["","","","Vidutinis","m³/min.","8.2"]
["","","","Mažas","m³/min.","6.2"]
["","","","Tylus veikimas","m³/min.","5.1"]
["","","Aušinimas","Mažas","m³/min.","5.7"]
["","","","Vidutinis","m³/min.","7.5"]
["","","","Didelis","m³/min.","10.5"]
["","","","Tylus veikimas","m³/min.","4.3"]
["Power supply","Fazė","","","","1~"]
["","Pavadinimas","","","","V1"]
["","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-240"]
["Pastabos","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m"]
["","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Šildymas","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Korpusas","Spalva","","","","","Balta","Balta","Balta","Balta","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","","295","295","295","295","295","295","299"]
["","","","Plotis","mm","","778","778","778","778","778","778","998"]
["","","","Gylis","mm","","272","272","272","272","272","272","292"]
["Svoris","Įrenginys","","","kg","","10","10","10","10","10","10","14.5"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Mažas","m³/min.","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Tylus veikimas","m³/min.","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Šildymas","Didelis","m³/min.","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","Šildymas","Mažas","m³/min.","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Tylus veikimas","m³/min.","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","58","58","58","58","58","58","58"]
["","Šildymas","","","dBA","","55","55","55","55","55","55","58"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","41","41","41","41","45","45","44"]
["","Vėsinimas","","Vidutinis","dBA","","33","33","33","33","33","33","40"]
["","","","Žemas","dBA","","25","25","25","25","25","25","36"]
["","","","Tylus veikimas","dBA","","19","19","19","19","19","19","27"]
["","Šildymas","","Aukštas","dBA","","39","39","39","39","39","39","43"]
["","","","Vidutinis","dBA","","34","34","34","34","35","35","39"]
["","","","Žemas","dBA","","26","26","27","27","28","28","34"]
["","","","Tylus veikimas","dBA","","20","20","20","20","20","20","31"]
["Vamzdžių jungtys","Skystis","","OD","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Drenažas","","","","","18","18","18","18","18","18","18"]
["Valdymo sistemos","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["El. tiekimas","Pavadinimas","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fazė","","","","","1~","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","","50","50","50","50","50","50","50"]
["","Įtampa","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standartiniai priedai","Silver particle filter","","","","","","","","","","","1"]