{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXTP-K"]
[]
[]
[]
[]
["","","","","","ATXTP25K3V1B","ATXTP35K3V1B"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.03","0.03"]
["","Šildymas","","Nom.","kW","0.035","0.035"]
["Korpusas","Spalva","","","","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","285","285"]
["","","","Plotis","mm","770","770"]
["","","","Gylis","mm","225","225"]
["Svoris","Įrenginys","","","kg","9","9"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","10.6","11.4"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7.7","8.2"]
["","","","Mažas","m³/min.","5.3","5.4"]
["","","","Tylus veikimas","m³/min.","4.3","4.3"]
["","","Šildymas","Didelis","m³/min.","11.2","10.8"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8","7.8"]
["","","Šildymas","Mažas","m³/min.","5.8","5.8"]
["","","","Tylus veikimas","m³/min.","4.9","4.9"]
["Garso galingumo lygis","Vėsinimas","","","dBA","58","58"]
["","Šildymas","","","dBA","58","58"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","43","43"]
["","Vėsinimas","","Vidutinis","dBA","35","35"]
["","","","Žemas","dBA","26","26"]
["","","","Tylus veikimas","dBA","21","21"]
["","Šildymas","","Aukštas","dBA","43","43"]
["","","","Vidutinis","dBA","35","35"]
["","","","Žemas","dBA","26","26"]
["","","","Tylus veikimas","dBA","21","21"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5"]
["","Drenažas","","","","16 (jungiamosios žarnos vidinis diametras)","16 (jungiamosios žarnos vidinis diametras)"]
["Kontrolės sistemos","Infrared remote control","","","","ARC480A11","ARC480A11"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["El. tiekimas","Pavadinimas","","","","V1","V1"]
["","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]