{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Aušinimo galingumas","Bendras galingumas","","Nom.","kW","12.10"]
["Šildymo galia","Bendras pajėgumas","","Nom.","kW","13.5"]
["Korpusas","Spalva","","","","Ryškiai balta"]
["Matmenys","Įrenginys","","Aukštis","mm","1850"]
["","","","Plotis","mm","600"]
["","","","Gylis","mm","350"]
["Svoris","Įrenginys","","","kg","50"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","28"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","26"]
["","","","Mažas","m³/min.","24"]
["","","Šildymas","Didelis","m³/min.","28"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","26"]
["","","Šildymas","Mažas","m³/min.","24"]
["Garso galingumo lygis","Vėsinimas","","","dBA","63"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","51"]
["","Vėsinimas","","Vidutinis","dBA","48"]
["","","","Žemas","dBA","46"]
["","Šildymas","","Aukštas","dBA","51"]
["","","","Vidutinis","dBA","46"]
["","","","Nom.","dBA","48"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52"]
["","Dujos","","Iš. diam.","mm","15.9"]
["","Drenažas","","","","I.D. 20/O.D. 26"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standartiniai priedai","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["El. tiekimas","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50/60"]
["","Įtampa","","","V","220-240/220"]