{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H52W"]
[]
[]
[]
[]
["","","","","BRC1H52W."]
["Pakuotė","Medžiaga","","","Kartonas"]
["","Svoris","","kg","0.0850"]
["Aplinkos temperatūra","Santykinis drėgnumas <","","%","95"]
["","Saugojimas","Min.","°C","-20"]
["","","Maks.","°C","70"]
["","Veikimas","Min.","°C","-10"]
["","","Maks.","°C","50"]
["Matmenys","Supakuotas įrenginys","Plotis","mm","217"]
["","","Aukštis","mm","50"]
["","","Gylis","mm","161"]
["","Įrenginys","Plotis","mm","85"]
["","","Gylis","mm","25"]
["","","Aukštis","mm","85"]
["Korpusas","Mygtuko dangtis","","","Ne"]
["","Spalva","","","Balta spalva"]
["","Veikimo LED","Spalva","","Blue status indicator"]
["LCD","Tipas","","","100 x 150 dots"]
["","Papildomas apšvietimas","Spalva","","Balta spalva"]
["","Matmenys","Plotis","mm","28.0"]
["","","Aukštis","mm","40.7"]
["Svoris","Supakuotas įrenginys","","kg","0.317"]
["","Įrenginys","","kg","0.110"]
["Laidų jungtys","Laidų ilgis","Maks.","m","500"]