{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW"]
["Korpusas","Spalva","","","Balta"]
["Korpusas| Mygtuko dangtis","","","","Ne"]
["Korpusas| Veikimo LED","Spalva","","","Mėlynas būsenos indikatorius"]
["Matmenys","Įrenginys","Aukštis","mm","85"]
["","","Plotis","mm","85"]
["","","Gylis","mm","25"]
["","Supakuotas įrenginys","Aukštis","mm","50"]
["","","Plotis","mm","217"]
["","","Gylis","mm","161"]
["Svoris","Įrenginys","","kg","0.110"]
["","Supakuotas įrenginys","","kg","0.317"]
["Pakuotė","Medžiaga","","","Kartonas"]
["","Svoris","","kg","0.0850"]
["LCD","Tipas","","","100 x 150 taškų"]
["Matmenys| Aukštis","mm","","","40.7"]
["Matmenys| Plotis","mm","","","28.0"]
["LCD","Papildomas apšvietimas| Spalva","","","Balta"]
["Aplinkos temperatūra","Veikimas","Min.","°C","-10"]
["","","Maks.","°C","52"]
["","Saugojimas","Min.","°C","-20"]
["","","Maks.","°C","70"]
["Aplinkos temperatūra| Santykinis drėgnumas <-=-%","%","","","95"]
["Valdymo sistemos","Temperatūros kontrolės klasė","","","VI"]
["Kontrolės sistemos","Įnašas į sezoninio erdvės šildymo efektyvumą","","%","4.0"]