{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","39"]
["","","Vidutinis","dBA","32"]
["","","Tylus veikimas","dBA","21"]
["","","Žemas","dBA","25"]
["","Aušinimas","Vidutinis","dBA","32"]
["","","Tylus veikimas","dBA","21"]
["","","Žemas","dBA","25"]
["","","Aukštas","dBA","39"]
["Standartiniai priedai","Įrengimo vadovas","","","1"]
["","Eksploatavimo vadovas","","","1"]
["","Oro filtras","","","2"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","1"]
["","Nuotolinio valdymo valdiklio montavimo plokštė","","","1"]
["","Sraigto maišas","","","1"]
["","Sraigto apdangalas","","","1"]
["","AAA sausosios baterijos","","","2"]
["","Bendrosios saugos priemonės","","","1"]
["Aušinimo medžiaga","GWP","","","675.0"]
["Valdymo sistemos","Wired remote control","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Piping connections","Skysčių vamzdis","OD","mm","6.35"]
["","Dujos","Iš. diam.","mm","9.50"]
["","Drenažo vamzdis","","","18"]
["Galios įvestis","Aušinimas","Nom.","kW","0.020"]
["","Šildymas","Nom.","kW","0.020"]
["Garso galingumo lygis","Vėsinimas","","dBA","57"]
["Matmenys","Vienetas","Plotis","mm","798"]
["","","Gylis","mm","189"]
["","","Aukštis","mm","295"]
["Korpusas","Colour","","","Afganistaninė akacija"]
["Svoris","Įrenginys","","kg","12"]
["Power supply","Phase","","","1~"]
["","Dažnis","","Hz","50"]
["","Pavadinimas","","","V1"]
["","Įtampa","","V","220-240"]