{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AW"]
[]
[]
[]
[]
["","","","","","CTXA15A2V1BW"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","39"]
["","","","Vidutinis","dBA","32"]
["","","","Tylus veikimas","dBA","21"]
["","","","Žemas","dBA","25"]
["","Aušinimas","","Vidutinis","dBA","32"]
["","","","Tylus veikimas","dBA","21"]
["","","","Žemas","dBA","25"]
["","","","Aukštas","dBA","39"]
["Standartiniai priedai","Įrengimo vadovas","","","","1"]
["","Eksploatavimo vadovas","","","","1"]
["","Oro filtras","","","","2"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","","1"]
["","Nuotolinio valdymo valdiklio montavimo plokštė","","","","1"]
["","Sraigto maišas","","","","1"]
["","Sraigto apdangalas","","","","1"]
["","AAA sausosios baterijos","","","","2"]
["","Bendrosios saugos priemonės","","","","1"]
["Aušinimo medžiaga","GWP","","","","675.0"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35"]
["","Dujos","","Iš. diam.","mm","9.50"]
["","Drenažo vamzdis","","","","18"]
["Power input","Aušinimas","","Nom.","kW","0.020"]
["","Šildymas","","Nom.","kW","0.020"]
["Sound power level","Vėsinimas","","","dBA","57"]
["Matmenys","Įrenginys","","Plotis","mm","798"]
["","","","Gylis","mm","189"]
["","","","Aukštis","mm","295"]
["Korpusas","Spalva","","","","Balta spalva"]
["Svoris","Įrenginys","","","kg","12"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","10.9"]
["","","","Vidutinis","m³/min.","8.7"]
["","","","Mažas","m³/min.","6.4"]
["","","","Tylus veikimas","m³/min.","4.5"]
["","","Aušinimas","Mažas","m³/min.","6.1"]
["","","","Vidutinis","m³/min.","8"]
["","","","Didelis","m³/min.","11.0"]
["","","","Tylus veikimas","m³/min.","4.6"]
["Power supply","Fazė","","","","1~"]
["","Pavadinimas","","","","V1"]
["","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-240"]