{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BS"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BS"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.02"]
["","Šildymas","","Nom.","kW","0.02"]
["Korpusas","Spalva","","","","Sidabrinė spalva"]
["Matmenys","Įrenginys","","Aukštis","mm","295"]
["","","","Plotis","mm","798"]
["","","","Gylis","mm","189"]
["Svoris","Įrenginys","","","kg","11.5"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","11"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","8.2"]
["","","","Mažas","m³/min.","6.1"]
["","","","Tylus veikimas","m³/min.","4.6"]
["","","Šildymas","Didelis","m³/min.","10.9"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.7"]
["","","Šildymas","Mažas","m³/min.","6.4"]
["","","","Tylus veikimas","m³/min.","4.5"]
["Garso galingumo lygis","Vėsinimas","","","dBA","57"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","39"]
["","Vėsinimas","","Vidutinis","dBA","32"]
["","","","Žemas","dBA","25"]
["","","","Tylus veikimas","dBA","21"]
["","Šildymas","","Aukštas","dBA","39"]
["","","","Vidutinis","dBA","32"]
["","","","Žemas","dBA","25"]
["","","","Tylus veikimas","dBA","21"]
["Aušinimo medžiaga","GWP","","","","675"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35"]
["","Dujos","","Iš. diam.","mm","9.5"]
["","Drenažas","","","","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARC466A58"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC073"]
["Standartiniai priedai","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Air filter","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["El. tiekimas","Pavadinimas","","","","V1"]
["","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-240"]