{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B (Archived)","CTXM15R5V1B (Archived)"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.029","0.029"]
["","Šildymas","","Nom.","kW","0.023","0.023"]
["Korpusas","Spalva","","","","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","295","295"]
["","","","Plotis","mm","778","778"]
["","","","Gylis","mm","272","272"]
["Svoris","Įrenginys","","","kg","10","10"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","10.5","10.5"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7.5","7.5"]
["","","","Mažas","m³/min.","5.7","5.7"]
["","","","Tylus veikimas","m³/min.","4.3","4.3"]
["","","Šildymas","Didelis","m³/min.","9.3","9.3"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.2","8.2"]
["","","Šildymas","Mažas","m³/min.","6.2","6.2"]
["","","","Tylus veikimas","m³/min.","5.1","5.1"]
["Garso galingumo lygis","Vėsinimas","","","dBA","57","57"]
["","Šildymas","","","dBA","54","54"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","41","41"]
["","Vėsinimas","","Vidutinis","dBA","33","33"]
["","","","Žemas","dBA","25","25"]
["","","","Tylus veikimas","dBA","19","19"]
["","Šildymas","","Aukštas","dBA","39","39"]
["","","","Vidutinis","dBA","34","34"]
["","","","Žemas","dBA","26","26"]
["","","","Tylus veikimas","dBA","20","20"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5"]
["","Drenažas","","","","18","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARC466A67","ARC466A67"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1","BRC073A1"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","1"]
["","Belaidis nuotolinis valdymas","","","","1","1"]
["","AAA sausosios baterijos","","","","2","2"]
["","WLAN adapterio rinkinys","","","","1","1"]
["","Eksploatavimo vadovas","","","","1","1"]
["","Dezodoruojantis filtras iš titano ir apatito","","","","1","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","2","2"]
["","Pritvirtinimo plokštė","","","","1","1"]
["","Nuotolinio valdymo pulto laikiklis","","","","1","1"]
["Energijos naudojimo efektyvumo klasė","","","","","A+++ ~ D","A+++ ~ D"]
["El. tiekimas","Pavadinimas","","","","V1","V1"]
["","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]
["Pastabos","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m"]
["","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m"]