{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","38","","41"]
["","","","Tylus veikimas","dBA","21","","21"]
["","","","Žemas","dBA","28","","30"]
["","Aušinimas","","Tylus veikimas","dBA","21","","21"]
["","","","Žemas","dBA","25","","28"]
["","","","Aukštas","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Aušinimas","","Nom.","dBA","31","","35"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","","1"]
["","Eksploatavimo vadovas","","","","1","","1"]
["","Belaidis nuotolinis valdymas","","","","1","","1"]
["","Elementai","","","","2","","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","1","","1"]
["","Pritvirtinimo plokštė","","","","1","","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","2","","2"]
["","Titano apatito fotokatalizatoriaus oro gryninimo filtras","","","","2","","2"]
["Kontrolės sistemos","Nuotolinis valdymas infraraudonaisiais spinduliais","","","","ARC466A6","","ARC466A6"]
["Vamzdžių jungtys","Skysčių vamzdis","","OD","mm","6.35","","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","","9.5"]
["","Drenažo vamzdis","","","","18","","18"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.040","","0.040"]
["","Šildymas","","Nom.","kW","0.040","","0.040"]
["Garso galingumo lygis","Vėsinimas","","","dBA","55","","59"]
["","Šildymas","","","dBA","56","","58"]
["Matmenys","Vienetas","","Plotis","mm","780","","780"]
["","","","Gylis","mm","215","","215"]
["","","","Aukštis","mm","289","","289"]
["Casing","Colour","","","","Balta spalva","","Balta spalva"]
["Svoris","Vienetas","","","kg","8","","8"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","","","10.1"]
["","","","Mažas","m³/min.","","","6.3"]
["","","","Tylus veikimas","m³/min.","","","4.3"]
["","","Aušinimas","Mažas","m³/min.","","","5.2"]
["","","","Didelis","m³/min.","","","9.2"]
["","","","Tylus veikimas","m³/min.","","","3.9"]
["","","","Nom.","m³/min.","","","8.1"]
["","","Aušinimas","Nom.","m³/min.","","","7.2"]
["Power supply","Fazė","","","","1~","","1~"]
["","Dažnis","","","Hz","50","","50"]
["","Pavadinimas","","","","V1","","V1"]
["","Įtampa","","","V","220-240","","220-240"]
["Pastabos","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","0.04","","0.040"]
["","Šildymas","","Nom.","kW","","0.04","","0.040"]
["Korpusas","Spalva","","","","","Balta","","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","","289","","289"]
["","","","Plotis","mm","","780","","780"]
["","","","Gylis","mm","","215","","215"]
["Svoris","Įrenginys","","","kg","","8","","8.00"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","7.9","","9.2"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","6.3","","7.2"]
["","","","Mažas","m³/min.","","4.7","","5.2"]
["","","","Tylus veikimas","m³/min.","","3.9","","3.9"]
["","","Šildymas","Didelis","m³/min.","","9","","10.1"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","7.5","","8.1"]
["","","Šildymas","Mažas","m³/min.","","6","","6.3"]
["","","","Tylus veikimas","m³/min.","","4.3","","4.3"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","55","","59"]
["","Šildymas","","","dBA","","56","","58"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","37","","42"]
["","Vėsinimas","","Vidutinis","dBA","","31","","35"]
["","","","Žemas","dBA","","25","","28"]
["","","","Tylus veikimas","dBA","","21","","21"]
["","Šildymas","","Aukštas","dBA","","38","","41"]
["","","","Vidutinis","dBA","","33","","36"]
["","","","Žemas","dBA","","28","","30"]
["","","","Tylus veikimas","dBA","","21","","21"]
["Vamzdžių jungtys","Skystis","","OD","mm","","6.35","","6.35"]
["","Dujos","","Iš. diam.","mm","","9.5","","9.50"]
["","Drenažas","","","","","18","","18"]
["Kontrolės sistemos","Nuotolinis valdymas infraraudonaisiais spinduliais","","","","","ARC466A6","","ARC466A6"]
["Standartiniai priedai","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["El. tiekimas","Pavadinimas","","","","","V1","","V1"]
["","Fazė","","","","","1~","","1~"]
["Maitinimas","Dažnis","","","Hz","","50","","50"]
["","Įtampa","","","V","","220-240","","220-240"]