{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBBH-D9W / ERLA-DV37"]
[]
[]
[]
[]
["","","","","","EBBH16DF9W / ERLA16DAV37","EBBH16DF9W / ERLA16D2V37"]
["Šildymo galingumas","Nom.","","","kW","16.0 (2) (1)","16.0 (1) (2)"]
["Tiekiama galia","Šildymas","","Nom.","kW","3.53 (1), 4.56 (2)","3.53 (1), 4.56 (2)"]
["COP","","","","","4.53 (1), 3.51 (2)","4.53 (1), 3.51 (2)"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.32","3.32"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.61","4.61"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++"]
["Pastabos","","","","","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(3) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(4) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(4) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","","(5) - Matuojamas, esant šildymo sistemoje 10 kPa slėgio kritimui tokiomis darbinėmis sąlygomis, kai patalpoje ištekančio vandens temperatūra yra 47–55 °C, o aplinkos – 20 °C. DB / WB 7 °C / 6°.","(5) - Matuojamas, esant šildymo sistemoje 10 kPa slėgio kritimui tokiomis darbinėmis sąlygomis, kai patalpoje ištekančio vandens temperatūra yra 47–55 °C, o aplinkos – 20 °C. DB / WB 7 °C / 6°."]