{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLA04-08E3V3"]
[]
[]
[]
[]
["","","","","","EBLA04E23V3","EBLA06E23V3","EBLA08E23V3"]
["Šildymo galingumas","Nom.","","","kW","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)"]
["Aušinimo galingumas","Nom.","","","kW","4.86 (1), 4.52 (2)","5.83 (1), 5.09 (2)","6.18 (1), 5.44 (2)"]
["Šildytuvo galingumas","1 veiksmas","","","kW","3","3","3"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.820 (1), 1.36 (2)","1.08 (1), 1.55 (2)","1.19 (1), 1.73 (2)"]
["","Šildymas","","Nom.","kW","0.840 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["EER","","","","","5.91 (1), 3.32 (2)","5.40 (1), 3.28 (2)","5.19 (1), 3.14 (2)"]
["Matmenys","Įrenginys","","Aukštis","mm","770","770","770"]
["","","","Plotis","mm","1250","1250","1250"]
["","","","Gylis","mm","362","362","362"]
["Svoris","Įrenginys","","","kg","91","91","91"]
["Veikimo diapazonas","Šildymas","Vandens pusė","Min.","°C","15 (3)","15 (3)","15 (3)"]
["","","","Maks.","°C","65 (3)","65 (3)","65 (3)"]
["","Aušinimas","Aplinkos","Min.","°CDB","10 (3)","10 (3)","10 (3)"]
["","","","Maks.","°CDB","43","43","43"]
["","","Vandens pusė","Min.","°C","5 (3)","5 (3)","5 (3)"]
["","","","Maks.","°C","22","22","22"]
["","Karštas buitinis vanduo","Aplinkos","Min.","°CDB","-27","-27","-27"]
["","","","Maks.","°CDB","35","35","35"]
["","","Vandens pusė","Min.","°C","25","25","25"]
["","","","Maks.","°C","55 (3)","55 (3)","55 (3)"]
["Garso galingumo lygis","Šildymas","","Nom.","dBA","58.0 (1)","60.0 (1)","62.0 (1)"]
["","Aušinimas","","Nom.","dBA","61.0 (1)","62.0 (1)","62.0 (1)"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","44.0 (1)","47.0 (1)","49.0 (1)"]
["","Aušinimas","","Nom.","dBA","48.0 (1)","49.0 (1)","50.0 (1)"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","GWP","","","","675","675","675"]
["","Užpildytas kiekis","","","kg","1.35","1.35","1.35"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.91","0.91","0.91"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.29","3.28","3.35"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.54","4.52","4.61"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++","A+++"]
["Kompresoriaus komponentas","Pagrindinis maitinimas","","Fazė","","3N~","3N~","3N~"]
["","","","Įtampa","V","220","220","220"]
["El. tiekimas","Pavadinimas","","","","V3","V3","V3"]
["","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","230 +/-10%","230 +/-10%","230 +/-10%"]
["Pastabos","","","","","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje"]