{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSH-D"]
[]
[]
[]
[]
["","","","","","EBSH11P30DG","EBSH11P50DG","EBSH16P30DG","EBSH16P50DG","EBSH11P30DF (Archived)","EBSH11P50DF (Archived)","EBSH16P30DF (Archived)","EBSH16P50DF (Archived)"]
["Korpusas","Spalva","","","","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)"]
["","Medžiaga","","","","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas"]
["Matmenys","Įrenginys","","Aukštis","mm","1893","1910","1893","1910","1893","1910","1893","1910"]
["","","","Plotis","mm","594","792","594","792","594","792","594","792"]
["","","","Gylis","mm","680","817","680","817","680","817","680","817"]
["Svoris","Įrenginys","","","kg","93","114","93","114","93","114","93","114"]
["PED","Kategorija","","","","II kategorija","II kategorija","II kategorija","II kategorija","II kategorija","II kategorija","II kategorija","II kategorija"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Užpildytas kiekis","","","kg","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["Šaltnešis","Užpildas","","","tCO2Eq","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Garso galingumo lygis","Nom.","","","dBA","44.7","44.7","49.0","49.0","44.7","44.7","49.0","49.0"]
["Garso slėgio lygis","Nom.","","","dBA","36.8","36.8","40.3","40.3","36.8","36.8","40.3","40.3"]
["Veikimo diapazonas","Šildymas","Vandens pusė","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Aušinimas","Aplinkos","Min.","°CDB","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Vandens pusė","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50","50","50"]
["","Įtampa","","","V","230","230","230","230","230","230","230","230"]
["Pastabos","","","","","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897"]
["","","","","","(2) - Žiūrėkite brėžinio darbines ribas","(2) - Žiūrėkite brėžinio darbines ribas","(2) - Žiūrėkite brėžinio darbines ribas","(2) - Žiūrėkite brėžinio darbines ribas","(2) - Žiūrėkite brėžinio darbines ribas","(2) - Žiūrėkite brėžinio darbines ribas","(2) - Žiūrėkite brėžinio darbines ribas","(2) - Žiūrėkite brėžinio darbines ribas"]