{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBVH-UD6V / ERLA-DW17"]
[]
[]
[]
[]
["","","","","","EBVH16SU23DJ6V / ERLA16D2W17","EBVH16SU23DJ6V / ERLA16DAW17"]
["Šildymo galingumas","Nom.","","","kW","16.0 (2) (1)","16.0 (2) (1)"]
["Tiekiama galia","Šildymas","","Nom.","kW","3.53 (1), 4.56 (2)","3.53 (1), 4.56 (2)"]
["Tiekiamas galingumas","Buitinio karšto vandens temperatūra nuo 10°C iki 50 °C","","Nom.","kWh","3.41","3.41"]
["Pašildymo iki temperatūros nuo 10°C iki 50 °C trukmė","val.","","","","1 val. 25 min., esant 7 °C aplinkos temperatūrai","1 val. 25 min., esant 7 °C aplinkos temperatūrai"]
["COP","","","","","4.53 (1), 3.51 (2)","4.53 (1), 3.51 (2)"]
["Buitinio karšto vandens išgavimas","Bendrai","","Nurodytos apkrovos profilis","","XL","XL"]
["Buitinio karšto vandens paruošimas","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","A","A"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.32","3.32"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.61","4.61"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++"]
["Energijos naudojimo efektyvumo klasė","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Pastabos","","","","","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(5) - Pagal EN14825","(5) - Pagal EN14825"]
["","","","","","(6) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(6) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(7) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(7) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","","(8) - Matuojamas, esant šildymo sistemoje 10 kPa slėgio kritimui tokiomis darbinėmis sąlygomis, kai patalpoje ištekančio vandens temperatūra yra 47–55 °C, o aplinkos – 20 °C. DB / WB 7 °C / 6°.","(8) - Matuojamas, esant šildymo sistemoje 10 kPa slėgio kritimui tokiomis darbinėmis sąlygomis, kai patalpoje ištekančio vandens temperatūra yra 47–55 °C, o aplinkos – 20 °C. DB / WB 7 °C / 6°."]