{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EDLA09-14D3W1"]
[]
[]
[]
[]
["","","","","","EDLA09DA3W1","EDLA11DA3W1","EDLA14DA3W1"]
["Šildymo galingumas","Nom.","","","kW","9.37 (1), 9.00 (2)","10.6 (1), 9.82 (2)","12.0 (1), 12.5 (2)"]
["Šildytuvo galingumas","1 veiksmas","","","kW","3","3","3"]
["Tiekiama galia","Šildymas","","Nom.","kW","1.91 (1), 2.43 (2)","2.18 (1), 2.68 (2)","2.46 (1), 3.42 (2)"]
["COP","","","","","4.91 (1), 3.71 (2)","4.83 (1), 3.66 (2)","4.87 (1), 3.64 (2)"]
["Matmenys","Įrenginys","","Aukštis","mm","870","870","870"]
["","","","Plotis","mm","1380","1380","1380"]
["","","","Gylis","mm","460","460","460"]
["Svoris","Įrenginys","","","kg","149","149","149"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","48.0","55.8","70.4"]
["Veikimo diapazonas","Šildymas","Vandens pusė","Min.","°C","15 (6)","15 (6)","15 (6)"]
["","","","Maks.","°C","60 (6)","60 (6)","60 (6)"]
["","Karštas buitinis vanduo","Aplinkos","Min.","°CDB","-25","-25","-25"]
["","","","Maks.","°CDB","35","35","35"]
["","","Vandens pusė","Min.","°C","25","25","25"]
["","","","Maks.","°C","55 (6)","55 (6)","55 (6)"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","GWP","","","","675","675","675"]
["","Užpildytas kiekis","","","kg","3.80","3.80","3.80"]
["Šaltnešis","Užpildas","","","tCO2Eq","2.57","2.57","2.57"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.39","3.32","3.37"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.72","4.64","4.62"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++","A+++"]
["Energijos naudojimo efektyvumo klasė","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Kompresoriaus komponentas","Pagrindinis maitinimas","","Fazė","","3N","3N~","3N~"]
["","","","Įtampa","V","400","400","400"]
["El. tiekimas","Pavadinimas","","","","W1","W1","W1"]
["","Fazė","","","","3~","3~","3~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","400","400","400"]
["Pastabos","","","","","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje"]
["","","","","","(4) - Priklauso nuo darbinio režimo, žr. įrengimo vadovą.","(4) - Priklauso nuo darbinio režimo, žr. įrengimo vadovą.","(4) - Priklauso nuo darbinio režimo, žr. įrengimo vadovą."]