{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Garso slėgio lygis","Nom.","","","dBA","32.0 (6)"]
["Aušinimo medžiaga","GWP","","","","2,090"]
["","Užpildytas kiekis","","","kg","1.80"]
["","Tipas","","","","R-410A"]
["Veikimo diapazonas","Montavimo vieta","","Min.","°C","5.00"]
["","","","Maks.","°C","30.0"]
["","Šildymas","Vandens pusė","Maks.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Sūraus vandens šonas","","Min.","°C","-5.00"]
["","","","Maks.","°C","20.0"]
["","Karštas buitinis vanduo","Vandens pusė","Maks.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Power input","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Sound power level","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Matmenys","Įrenginys","","Plotis","mm","600"]
["","","","Gylis","mm","728"]
["","","","Aukštis","mm","1,730"]
["Casing","Material","","","","Apsaugine danga dengtas lakštinis metalas"]
["","Spalva","","","","Balta spalva"]
["Bakas","Vandens tūris","","","l","180"]
["","Apsauga nuo korozijos","","","","Anodas"]
["","Izoliacija","","Šiluminiai nuostoliai","kWh/24h","1.36 (4)"]
["Weight","Įrenginys","","","kg","210"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 35 °C","Bendrai","ηs (sezoninio erdvinio šildymo efektyvumas)","%","194"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A+++"]
["","","","SCOP","","5.06"]
["","Average climate water outlet 55°C","Bendrai","Seasonal space heating eff. class","","A++"]
["","","","ηs (sezoninio erdvinio šildymo efektyvumas)","%","139"]
["","","","SCOP","","3.68"]
["Šildymo galingumas","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Maks.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Phase","","","","3~"]
["","Pavadinimas","","","","9W"]
["","Dažnis","","","Hz","50"]
["","Įtampa","","","V","400"]
["Srovė","Rekomenduojami lydieji saugikliai","","","A","25"]
["Pastabos","","","","","(1) - EWB/LWB 0 °C/-3 °C - LWC 35 °C (DT=5 °C)"]
["","","","","","(2) - EWB/LWB 0 °C/-3 °C - LWC 45 °C (DT=5 °C)"]
["","","","","","(3) - su 40 % propileno glikoliu"]
["","","","","","(4) - Šilumos nuostoliai pagal EN12897"]
["","","","","","(5) - įskaitant vamzdyną + PHE + atsarginį šildytuvą; išskyrus plėtimosi indą"]
["","","","","","(6) - Triukšmo lygis matuojamas naudojant mikrofoną 1 m atstumu nuo prietaiso. Ši vertė yra santykinė ir priklauso nuo atstumo bei akustinės aplinkos."]
["","","","","","(7) - Šiluminiu siurbliu"]
["","","","","","(8) - Šiluminiu siurbliu + atsarginiu šildytuvu"]
["","","","","","(9) - Atsarginiu šildytuvu"]