{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":11,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3 / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3 / ERGA04EAV3A","EHSX04P50DA3 / ERGA04EAV3A","EHSX08P30DA3 / ERGA06EAV3A","EHSX08P50DA3 / ERGA06EAV3A","EHSX08P30DA3 / ERGA08EAV3A","EHSX08P50DA3 / ERGA08EAV3A"]
["Indoor unit","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Šildymo galingumas","Nom.","","","kW","4.30, 4.60","4.30, 4.60","6.00, 5.90","6.00, 5.90","7.50, 7.80","7.50, 7.80"]
["Aušinimo galingumas","Nom.","","","kW","4.86, 4.52","4.86, 4.52","5.96, 5.09","5.96, 5.09","6.25, 5.44","6.25, 5.44"]
["Tiekiama galia","Šildymas","","Nom.","kW","0.840, 1.26","0.840, 1.26","1.24, 1.69","1.24, 1.69","1.63, 2.23","1.63, 2.23"]
["","Aušinimas","","Nom.","kW","0.810, 1.36","0.810, 1.36","1.06, 1.55","1.06, 1.55","1.16, 1.73","1.16, 1.73"]
["COP","","","","","5.10, 3.65","5.10, 3.65","4.85, 3.50","4.85, 3.50","4.60, 3.50","4.60, 3.50"]
["EER","","","","","5.98, 3.32","5.98, 3.32","5.61, 3.28","5.61, 3.28","5.40, 3.14","5.40, 3.14"]
["Buitinio karšto vandens išgavimas","Bendrai","","Nurodytos apkrovos profilis","","L","XL","L","XL","L","XL"]
["Buitinio karšto vandens paruošimas","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","A+","A","A+","A","A+","A"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.29","3.29","3.27","3.27","3.30","3.30"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++","A++","A++","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.54","4.54","4.52","4.52","4.61","4.61"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Pastabos","","","","","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]