{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Korpusas","Spalva","","","","Baltas (RAL9010) / tamsiai pilkas (RAL7011)","Baltas (RAL9010) / tamsiai pilkas (RAL7011)","Baltas (RAL9010) / tamsiai pilkas (RAL7011)","Baltas (RAL9010) / tamsiai pilkas (RAL7011)"]
["","Medžiaga","","","","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas"]
["Matmenys","Įrenginys","","Aukštis","mm","1891","1896","1891","1896"]
["","","","Plotis","mm","595","790","595","790"]
["","","","Gylis","mm","615","790","615","790"]
["Svoris","Įrenginys","","","kg","73.0","93.0","73.0","93.0"]
["PED","Kategorija","","","","užs. 3.3","užs. 3.3","užs. 3.3","užs. 3.3"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0","675.0","675.0"]
["","Užpildytas kiekis","","","kg","1.50","1.50","1.50","1.50"]
["Garso galingumo lygis","Nom.","","","dBA","39","39","39","39"]
["Veikimo diapazonas","Šildymas","Vandens pusė","Min.","°C","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65"]
["","Aušinimas","Aplinkos","Min.","°C DB","10","10","10","10"]
["","","Vandens pusė","Min.","°C","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50"]
["","Įtampa","","","V","230","230","230","230"]
["Elektrinis šildytuvas","Maitinimas","","Pavadinimas","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Fazė","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Dažnis","Hz","50","50","50","50"]
["Pastabos","","","","","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897"]
["","","","","","(2) - TKW = 10 °C / TWW = 40 °C / TSP = 50 °C","(2) - TKW = 10 °C / TWW = 40 °C / TSP = 50 °C","(2) - TKW = 10 °C / TWW = 40 °C / TSP = 50 °C","(2) - TKW = 10 °C / TWW = 40 °C / TSP = 50 °C"]
["","","","","","(3) - TKW = 10 °C / TWW = 40 °C / TSP = 60 °C","(3) - TKW = 10 °C / TWW = 40 °C / TSP = 60 °C","(3) - TKW = 10 °C / TWW = 40 °C / TSP = 60 °C","(3) - TKW = 10 °C / TWW = 40 °C / TSP = 60 °C"]
["","","","","","(4) - TKW = 10 °C / TWW = 40 °C / TSP = 65 ℃","(4) - TKW = 10 °C / TWW = 40 °C / TSP = 65 ℃","(4) - TKW = 10 °C / TWW = 40 °C / TSP = 65 ℃","(4) - TKW = 10 °C / TWW = 40 °C / TSP = 65 ℃"]
["","","","","","","(5) - Talpyklos įšildymas tik su šiluminiu siurbliu be elektrinio šildytuvo","","(5) - Talpyklos įšildymas tik su šiluminiu siurbliu be elektrinio šildytuvo"]