{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-E"]
[]
[]
[]
[]
["","","","","","EHSX04P30EF","EHSX04P30EG","EHSX04P50EF","EHSX04P50EG","EHSX08P30EF","EHSX08P30EG","EHSX08P50EF","EHSX08P50EG"]
["Korpusas","Spalva","","","","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)"]
["","Medžiaga","","","","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas"]
["Matmenys","Įrenginys","","Aukštis","mm","1892","1891","1905","1910","1892","1891","1905","1910"]
["","","","Plotis","mm","594","594","792","792","594","594","792","792"]
["","","","Gylis","mm","644","644","812","817","644","644","812","817"]
["Svoris","Įrenginys","","","kg","77","77.0","107","97.0","77","77.0","107","97.0"]
["PED","Kategorija","","","","Užs.4.3","Užs.4.3","Užs.4.3","Užs.4.3","Užs.4.3","Užs.4.3","Užs.4.3","Užs.4.3"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Aušinimo medžiaga","GWP","","","","675","675.0","675","675.0","675","675.0","675","675.0"]
["","Užpildytas kiekis","","","kg","1.5","1.50","1.5","1.50","1.5","1.50","1.5","1.50"]
["Garso galingumo lygis","Nom.","","","dBA","39","39","39","39","39","39","39","39"]
["Veikimo diapazonas","Šildymas","Vandens pusė","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65","65","65","65","65"]
["","Aušinimas","Aplinkos","Min.","°C DB","10","10","10","10","10","10","10","10"]
["","","Vandens pusė","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22","22","22","22","22"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50","50","50"]
["","Įtampa","","","V","230","230","230","230","230","230","230","230"]
["Pastabos","","","","","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897","(1) - Šilumos nuostoliai pagal EN12897"]