{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-E6V / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHVZ08S18EA6V / ERGA08EAV3H7","EHVZ08S18EJ6V / ERGA08EAV3H7","EHVZ08S23EA6V / ERGA08EAV3H7","EHVZ08S23EJ6V / ERGA08EAV3H7"]
["Šildymo galingumas","Nom.","","","kW","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Tiekiama galia","Šildymas","","Nom.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Tiekiamas galingumas","Buitinio karšto vandens temperatūra nuo 10°C iki 50 °C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Pašildymo iki temperatūros nuo 10°C iki 50 °C trukmė","hr","","","","1 h 28 min","1 h 28 min","1 h 40 min","1 h 40 min"]
["COP","","","","","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Buitinio karšto vandens išgavimas","Bendrai","","Nurodytos apkrovos profilis","","L","L","XL","XL"]
["Buitinio karšto vandens paruošimas","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","A+","A+","A+","A+"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.56","4.56","4.56","4.56"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++","A+++","A+++"]
["Energijos naudojimo efektyvumo klasė","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Pastabos","","","","","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]