{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":9,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV32 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBH05AAV32 / EVLQ05CAV3","EHYHBH05AFV32 / EVLQ05CAV3","EHYHBH08AAV32 / EVLQ08CAV3","EHYHBH08AFV32 / EVLQ08CAV3"]
["Buitinio karšto vandens šildymas","Bendra","","Nurodytos apkrovos profilis","","XL"]
["","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","A"]
["COP","","","","","5.04 (1), 3.58 (2)","5.04, 3.58","4.45, 3.42","4.45, 3.42"]
["Šildymo galingumas","Nom.","","","kW","4.40 (1), 4.03 (2)"]
["","Min.","","","kW","1.80 (1), 1.80 (2)"]
["","Maks.","","","kW","5.12 (1), 4.90 (2)"]
["Galios įvestis","Šildymas","","Nom.","kW","0.870 (1), 1.13 (2)"]
["Pastabos","","","","","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(3) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C), boileris apeinamas","(3) - DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C), boileris apeinamas","(3) - DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C), boileris apeinamas"]
["","","","","","(4) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(4) - DB/WB 7 °C/6 °C – LWC 45 ℃ (DT = 5 °C), boileris apeinamas","(4) - DB/WB 7 °C/6 °C – LWC 45 ℃ (DT = 5 °C), boileris apeinamas","(4) - DB/WB 7 °C/6 °C – LWC 45 ℃ (DT = 5 °C), boileris apeinamas"]
["","","","","","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C), virintuvas apeinamas"]
["","","","","","(6) - Tamb 35 °C - LWE 18 ℃ (DT=5 °C), virintuvas apeinamas"]
["","","","","","(7) - DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C), boileris apeinamas"]
["","","","","","(8) - DB/WB 7 °C/6 °C – LWC 45 ℃ (DT = 5 °C), boileris apeinamas"]
["Šildymo galingumas","Min.","","","kW","","1.80, 1.80","1.80, 1.80","1.80, 1.80"]
["","Nom.","","","kW","","4.40, 4.03","7.40, 6.89","7.40, 6.89"]
["","Maks.","","","kW","","5.12, 4.90","10.0, 9.53","10.0, 9.53"]
["Tiekiama galia","Šildymas","","Nom.","kW","","0.870, 1.13","1.66, 2.01","1.66, 2.01"]
["Buitinio karšto vandens išgavimas","Bendrai","","Nurodytos apkrovos profilis","","","XL","XL","XL"]
["Buitinio karšto vandens paruošimas","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","","A","A","A"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","","3.28","3.24","3.24"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","","A++","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","","4.50","4.25","4.25"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","","A+++","A++","A++"]