{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AAV3 / EVLQ08CAV3","EHYHBX08AFV3 / EVLQ08CAV3"]
["Buitinio karšto vandens paruošimas","Bendra","","Nurodytos apkrovos profilis","","XL"]
["","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","A"]
["COP","","","","","4.45 (3), 3.42 (4)","4.45, 3.42"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","Sezoninio erdvinio šildymo ef. klasė","","A++"]
["","","","ηs (sezoninio erdvinio šildymo efektyvumas)","%","129"]
["","","","SCOP","","3.29"]
["Aušinimo galingumas","Nom.","","","kW","6.86 (4), 5.36 (4)"]
["","Min.","","","kW","2.50 (3), 2.50 (4)"]
["EER","","","","","3.42 (3), 2.29 (4)","3.42, 2.29"]
["Šildymo galingumas","Nom.","","","kW","7.40 (3), 6.89 (4)"]
["","Min.","","","kW","1.80 (3), 1.80 (4)"]
["","Maks.","","","kW","10.0 (3), 9.53 (4)"]
["Power input","Aušinimas","","Nom.","kW","2.01 (3), 2.34 (4)"]
["","Šildymas","","Nom.","kW","1.66 (3), 2.01 (4)"]
["Pastabos","","","","","(1) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(2) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)"]
["","","","","","(3) - 1 sąlyga: aušinimas Ta 35 °C - LWE 18 °C (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT=5 °C), virintuvas apeinamas"]
["","","","","","(4) - 2 sąlyga: aušinimas Ta 35 °C - LWE 7℃ (Dt: = 5°C); šildymas Ta DB/WB 7 °C/6 °C - LWC 45℃ (DT = 5 °C)","(4) - Tamb 35 °C - LWE 18 ℃ (DT=5 °C), virintuvas apeinamas"]
["","","","","","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C), virintuvas apeinamas","(5) - DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C), boileris apeinamas"]
["","","","","","(6) - Tamb 35 °C - LWE 18 ℃ (DT=5 °C), virintuvas apeinamas","(6) - DB/WB 7 °C/6 °C – LWC 45 ℃ (DT = 5 °C), boileris apeinamas"]
["","","","","","(7) - DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C), boileris apeinamas"]
["","","","","","(8) - DB/WB 7 °C/6 °C – LWC 45 ℃ (DT = 5 °C), boileris apeinamas"]
["Šildymo galingumas","Min.","","","kW","","1.80, 1.80"]
["","Nom.","","","kW","","7.40, 6.89"]
["","Maks.","","","kW","","10.0, 9.53"]
["Aušinimo galingumas","Min.","","","kW","","2.50, 2.50"]
["","Nom.","","","kW","","6.86, 5.36"]
["Tiekiama galia","Šildymas","","Nom.","kW","","1.66, 2.01"]
["","Aušinimas","","Nom.","kW","","2.01, 2.34"]
["Buitinio karšto vandens išgavimas","Bendrai","","Nurodytos apkrovos profilis","","","XL"]
["Buitinio karšto vandens paruošimas","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","","A"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","","3.29"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","","4.28"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","","A++"]
["Energijos naudojimo efektyvumo klasė","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]