{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Korpusas","Spalva","","","","Balta"]
["","Medžiaga","","","","Apsaugine danga dengtas lakštinis metalas"]
["Matmenys","Įrenginys","","Aukštis","mm","902"]
["","","","Plotis","mm","450"]
["","","","Gylis","mm","164"]
["Svoris","Įrenginys","","","kg","31.2"]
["PED","Kategorija","","","","I kategorija"]
["Vandens pusės šilumokaitis","Vandens srauto greitis","Šildymas","Maks.","l/min.","23.5 (7)"]
["Garso galingumo lygis","Nom.","","","dBA","42.0"]
["Veikimo diapazonas","Šildymas","Vandens pusė","Min.","°C","25 (8)"]
["","","","Maks.","°C","55 (8)"]
["","Aušinimas","Aplinkos","Min.","°CDB","10 (8)"]
["","","Vandens pusė","Min.","°C","5 (8)"]
["","","","Maks.","°C","22 (8)"]
["El. tiekimas","Pavadinimas","","","","V3"]
["","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50"]
["","Įtampa","","","V","230"]
["Laidų jungtys","Jungčiai su vartotojo sąsaja","","Kiekis","","2"]
["","","","Pastaba","","Nuo 0,75 mm² iki 1,25 mm² (maks. ilgis 500 m)"]
["Pastabos","","","","","(1) - Tik vidinio įrengimo"]
["","","","","","(2) - DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C), boileris apeinamas"]
["","","","","","(3) - DB/WB 7 °C/6 °C – LWC 45 ℃ (DT = 5 °C), boileris apeinamas"]
["","","","","","(4) - Tamb 35 °C - LWE 7 °C (DT=5 °C), virintuvas apeinamas"]
["","","","","","(5) - Tamb 35 °C - LWE 18 ℃ (DT=5 °C), virintuvas apeinamas"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Boileris apeinamas"]
["","","","","","(8) - *HYHB* ir *HYKOMB33AA darbinis diapazonas nurodomas darbinio diapazono brėžinyje"]