{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBX-E6V / ERRA-EW17"]
[]
[]
[]
[]
["","","","","","ELBX12EF6V / ERRA08EAW17","ELBX12EF6V / ERRA10EAW17","ELBX12EF6V / ERRA12EAW17"]
["Šildymo galingumas","Min.","","","kW","3.45 (1)","3.45 (1)","3.45 (1)"]
["","Nom.","","","kW","6.17 (2)","6.17 (2)","6.17 (2)"]
["","Maks.","","","kW","7.95 (1)","9.25 (1)","9.97 (1)"]
["Aušinimo galingumas","Nom.","","","kW","6.81 (3), 6.47 (4)","7.97 (3), 6.47 (4)","8.62 (3), 6.47 (4)"]
["Tiekiama galia","Šildymas","","Min.","kW","0.70 (5)","0.70 (5)","0.70 (5)"]
["","","","Nom.","kW","1.21 (2)","1.21 (2)","1.21 (2)"]
["","","","Maks.","kW","1.63 (5)","1.98 (5)","2.21 (5)"]
["","Aušinimas","","Nom.","kW","2.08 (3), 1.13 (4)","2.57 (3), 1.13 (4)","2.86 (3), 1.13 (4)"]
["COP","","","","","5.10 (2)","5.10 (2)","5.10 (2)"]
["EER","","","","","3.28 (3), 5.75 (4)","5.75 (4)","3.01 (3), 5.75 (4)"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.58","3.58","3.58"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.95","4.98","4.98"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++","A+++"]
["Energijos naudojimo efektyvumo klasė","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Pastabos","","","","","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C"]
["","","","","","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511"]
["","","","","","(6) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu","(6) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu","(6) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu"]