{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSHB-E"]
[]
[]
[]
[]
["","","","","","ELSHB12P30EG","ELSHB12P50EG","ELSHB12P50EF (Archived)","ELSHB12P30EF (Archived)"]
["Korpusas","Spalva","","","","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)","Balta (RAL9016) / juoda (RAL9017)"]
["","Medžiaga","","","","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas","Smūgiams atsparus polipropilenas"]
["Matmenys","Įrenginys","","Aukštis","mm","1891","1910","1910","1893"]
["","","","Plotis","mm","594","792","792","594"]
["","","","Gylis","mm","680","817","817","680"]
["Svoris","Įrenginys","","","kg","93.0","115","91.0","76.0"]
["PED","Kategorija","","","","II kategorija","II kategorija","II kategorija","II kategorija"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32"]
["Garso galingumo lygis","Nom.","","","dBA","44.7","44.7","44.7","44.7"]
["Garso slėgio lygis","Nom.","","","dBA","36.8","36.8","36.8","36.8"]
["Veikimo diapazonas","Šildymas","Vandens pusė","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Maks.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Aušinimas","Aplinkos","Min.","°CDB","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Vandens pusė","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Maks.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50"]
["","Įtampa","","","V","230","230","230","230"]
["Pastabos","","","","","(1) - Darbinė sritis pratęsiama iki žemesnio srauto koeficientų, atsižvelgiant į darbinį režimą – žiūrėkite ESP kreivę.","(1) - Darbinė sritis pratęsiama iki žemesnio srauto koeficientų, atsižvelgiant į darbinį režimą – žiūrėkite ESP kreivę.","(1) - Darbinė sritis pratęsiama iki žemesnio srauto koeficientų, atsižvelgiant į darbinį režimą – žiūrėkite ESP kreivę.","(1) - Darbinė sritis pratęsiama iki žemesnio srauto koeficientų, atsižvelgiant į darbinį režimą – žiūrėkite ESP kreivę."]
["","","","","","(2) - Šilumos nuostoliai pagal EN12897","(2) - Šilumos nuostoliai pagal EN12897","(2) - Šilumos nuostoliai pagal EN12897","(2) - Šilumos nuostoliai pagal EN12897"]
["","","","","","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(3) - Daugiau informacijos rasite veikimo diapazono brėžinyje"]