{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELVX-E6V / ERRA08-12EW1"]
[]
[]
[]
[]
["","","","","","ELVX12S18EJ6V / ERRA08EAW1","ELVX12S23EJ6V / ERRA08EAW1","ELVX12S18EJ6V / ERRA10EAW1","ELVX12S23EJ6V / ERRA10EAW1","ELVX12S18EJ6V / ERRA12EAW1","ELVX12S23EJ6V / ERRA12EAW1"]
["Šildymo galingumas","Min.","","","kW","3.45","3.45","3.45","3.45","3.45","3.45"]
["","Nom.","","","kW","6.17","6.17","6.17","6.17","6.17","6.17"]
["","Maks.","","","kW","7.95","7.95","9.25","9.25","9.97","9.97"]
["Aušinimo galingumas","Nom.","","","kW","6.81, 6.47","6.81, 6.47","7.97, 6.47","7.97, 6.47","8.62, 6.47","8.62, 6.47"]
["Tiekiama galia","Šildymas","","Min.","kW","0.70","0.70","0.70","0.70","0.70","0.70"]
["","","","Nom.","kW","1.21","1.21","1.21","1.21","1.21","1.21"]
["","","","Maks.","kW","1.63","1.63","1.98","1.98","2.21","2.21"]
["","Aušinimas","","Nom.","kW","2.08, 1.13","2.08, 1.13","2.57, 1.13","2.57, 1.13","2.86, 1.13","2.86, 1.13"]
["Tiekiamas galingumas","Buitinio karšto vandens temperatūra nuo 10°C iki 50 °C","","Nom.","kWh","2.54","3.09","2.54","3.09","2.54","3.09"]
["Pašildymo iki temperatūros nuo 10°C iki 50 °C trukmė","val.","","","","1 h 51 min","2 h 10 min","1 h 51 min","2 h 10 min","1 h 51 min","2 h 10 min"]
["COP","","","","","5.10","5.10","5.10","5.10","5.10","5.10"]
["EER","","","","","3.28, 5.75","3.28, 5.75","3.10, 5.75","3.10, 5.75","3.01, 5.75","3.01, 5.75"]
["Buitinio karšto vandens išgavimas","Bendrai","","Nurodytos apkrovos profilis","","L","L","L","L","L","L"]
["Buitinio karšto vandens paruošimas","Vidutinis klimatas","","Vandens šildymo energijos efektyvumo klasė","","A+","A+","A+","A+","A+","A+"]
["Erdvinis šildymas","Vid. klimato vandens išleidimo anga 55°C","Bendrai","SCOP","","3.47","3.47","3.48","3.48","3.58","3.58"]
["","","","Sezoninio erdvinio šildymo ef. klasė","","A++","A++","A++","A++","A++","A++"]
["","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-SCOP","","4.95","4.95","4.98","4.98","4.98","4.98"]
["","","","Erdvinis šildymas-=-Vid. klimato vandens išleidimo anga 35&nbsp;°C-=-Bendrai-=-Sezoninio erdvinio šildymo ef. klasė","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Pastabos","","","","","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C","(1) - Galia pagal standartą EN14511, taip pat galioja šilto vandens intervalui dT = 3~8 °C, kai Ta 7 °C"]
["","","","","","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(2) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(3) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(4) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511","(5) - Maitinimo įvestis – visa vidaus ir lauko įrenginių įvestis, įskaitant cirkuliacijos siurblį; pagal EN14511"]
["","","","","","(6) - Tikrinama, kai Ta DB / WB 7°C / 6 °C. Remiantis EN 16147.","(6) - Tikrinama, kai Ta DB / WB 7°C / 6 °C. Remiantis EN 16147.","(6) - Tikrinama, kai Ta DB / WB 7°C / 6 °C. Remiantis EN 16147.","(6) - Tikrinama, kai Ta DB / WB 7°C / 6 °C. Remiantis EN 16147.","(6) - Tikrinama, kai Ta DB / WB 7°C / 6 °C. Remiantis EN 16147.","(6) - Tikrinama, kai Ta DB / WB 7°C / 6 °C. Remiantis EN 16147."]
["","","","","","(7) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu","(7) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu","(7) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu","(7) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu","(7) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu","(7) - DB/WB 7 °C / 6 °C – LWC 35 °C (dT = 5 °C), siurbliui veikiant visu greičiu"]