{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","ERGA08EAV3H7"]
["Matmenys","Įrenginys","","Aukštis","mm","740"]
["","","","Plotis","mm","884"]
["","","","Gylis","mm","388"]
["Svoris","Įrenginys","","","kg","58.5"]
["Darb. inter.","Vėsinimas","","Min.","°C DB","10"]
["","","","Maks.","°C DB","43"]
["Veikimo diapazonas","Karštas buitinis vanduo","","Min.","°C DB","-25"]
["Darb. inter.","Karštas buitinis vanduo","","Maks.","°C DB","35"]
["Garso galingumo lygis","Šildymas","","Nom.","dBA","62 (1)"]
["","Aušinimas","","Nom.","dBA","62 (1)"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","49 (1)"]
["","Aušinimas","","Nom.","dBA","50 (1)"]
["Šaltnešis","Tipas","","","","R-32"]
["Aušinimo medžiaga","GWP","","","","675.0"]
["Šaltnešis","Užpildas","","","tCO2Eq","1.01"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.50"]
["Vamzdžių jungtys","Skystis","","OD","mm","6"]
["","Dujos","","Iš. diam.","mm","15.9"]
["","Drenažo vamzdis","","OD","mm","18"]
["","Lygio skirtumas","IU - OU","Maks.","m","30.0"]
["","Šilumos izoliacija","","","","Skysčio ir dujų vamzdžiai"]
["El. tiekimas","Pavadinimas","","","","V3"]
["","Fazė","","","","1N~"]
["Maitinimas","Dažnis","","","Hz","50"]
["","Įtampa","","","V","230"]
["Srovė","Rekomenduojami lydieji saugikliai","","","A","25"]
["Pastabos","","","","","(1) - Aušinimas Ta 35 °C - LWE 18 °C ( DT = 5 °C ) - šildymas Ta DB/WB 7 °C / 6 °C - LWC 35 °C ( DT = 5 °C )"]