{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Matmenys","Įrenginys","","Aukštis","mm","870","870"]
["","","","Plotis","mm","1,100","1,100"]
["","","","Gylis","mm","460","460"]
["Svoris","Įrenginys","","","kg","101","101"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","85.0","85.0"]
["","","Aušinimas","Didelis","m³/min.","85","85"]
["Darb. inter.","Vėsinimas","","Min.","°CDB","10","10"]
["","","","Maks.","°CDB","43","43"]
["Veikimo diapazonas","Karštas buitinis vanduo","","Min.","°CDB","-25","-25"]
["Darb. inter.","Karštas buitinis vanduo","","Maks.","°CDB","25 (1), 35 (1)","25 (1), 35 (1)"]
["Garso galingumo lygis","Šildymas","","Nom.","dBA","62.0 (2)","62.0 (2)"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","48.0 (2)","48.0 (2)"]
["Šaltnešis","Tipas","","","","R-32","R-32"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0"]
["Šaltnešis","Užpildas","","","tCO2Eq","2.57","2.57"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","3.8","3.8"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.5","9.5"]
["","Dujos","","Iš. diam.","mm","15.9","15.9"]
["","Drenažo vamzdis","","OD","mm","26","26"]
["","Lygio skirtumas","IU - OU","Maks.","m","30.0","30.0"]
["","Šilumos izoliacija","","","","Skysčio ir dujų vamzdžiai","Skysčio ir dujų vamzdžiai"]
["El. tiekimas","Pavadinimas","","","","W1","W1"]
["","Fazė","","","","3~","3~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","400","400"]
["Srovė","Rekomenduojami lydieji saugikliai","","","A","16","16"]
["Pastabos","","","","","(1) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(1) - Daugiau informacijos rasite veikimo diapazono brėžinyje"]
["","","","","","(2) - Matuojamas, esant šildymo sistemoje 10 kPa slėgio kritimui tokiomis darbinėmis sąlygomis, kai patalpoje ištekančio vandens temperatūra yra 47–55 °C, o aplinkos – 20 °C. DB / WB 7 °C / 6°.","(2) - Matuojamas, esant šildymo sistemoje 10 kPa slėgio kritimui tokiomis darbinėmis sąlygomis, kai patalpoje ištekančio vandens temperatūra yra 47–55 °C, o aplinkos – 20 °C. DB / WB 7 °C / 6°."]