{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWAA-DW1P-H"]
[]
[]
[]
[]
["","","","","","EWAA011DAW1P-H-","EWAA014DAW1P-H-","EWAA016DAW1P-H-"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","47.7","50.8","51.0"]
["Hidrauliniai komponentai","Plėtimosi indas","","Talpa","l","8","8","8"]
["Veikimo diapazonas","Oro pusė","Aušinimas","Min.","°CDB","10","10","10"]
["","","","Maks.","°CDB","43","43","43"]
["","Vandens pusė","Aušinimas","Maks.","°CDB","22","22","22"]
["","","","Min.","°CDB","5","5","5"]
["Šaltnešio užpild.","Grandinėje","","","kg","3.80","3.80","3.80"]
["","Grandinėje","","","TCO2Eq","2.6","2.6","2.6"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis inverterio kompresorius","Hermetiškai užsandarintas stūmoklinis inverterio kompresorius","Hermetiškai užsandarintas stūmoklinis inverterio kompresorius"]
["","Paleidimo metodas_","","","","Varomas inverterio","Varomas inverterio","Varomas inverterio"]
["","Kiekis_","","","","1","1","1"]
["Air heat exchanger","Tipas","","","","Didelio efektyvumo briaunos ir vamzdžio tipo su integruotu pagalbiniu aušintuvu","Didelio efektyvumo briaunos ir vamzdžio tipo su integruotu pagalbiniu aušintuvu","Didelio efektyvumo briaunos ir vamzdžio tipo su integruotu pagalbiniu aušintuvu"]
["Svoris","Įrenginys","","","kg","147","147","147"]
["EER","","","","","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0","675.0"]
["","Tipas","","","","R-32","R-32","R-32"]
["","Grandinės","","Kiekis","","1","1","1"]
["","Valdiklis","","","","Elektroninis plėtimosi vožtuvas","Elektroninis plėtimosi vožtuvas","Elektroninis plėtimosi vožtuvas"]
["Ventiliatoriaus variklis","Greitis","Aušinimas","Nom.","rpm","550","650","650"]
["Aušinimo galingumas","Nom.","","","kW","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Vandens šilumokaitis","Vandens tūris","","","l","2","2","2"]
["","Minimalus vandens tūris sistemoje","","","l","20 (6)","20 (6)","20 (6)"]
["","Tipas","","","","Plokštelinis šilumokaitis","Plokštelinis šilumokaitis","Plokštelinis šilumokaitis"]
["Power input","Aušinimas","","Nom.","kW","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["Sound power level","Aušinimas","","Nom.","dBA","67.0","69.0","69.0"]
["Matmenys","Įrenginys","","Plotis","mm","1,380","1,380","1,380"]
["","","","Gylis","mm","460","460","460"]
["","","","Aukštis","mm","870","870","870"]
["Galingumo valdymas","Būdas","","","","Kintanti (inverterio)","Kintanti (inverterio)","Kintanti (inverterio)"]
["Ventiliatorius","Oro debitas","Aušinimas","Nom.","m³/min.","70","85","85"]
["Kompresorius","Paleidimo metodas_","","","","Inverteris","Inverteris","Inverteris"]
["Power supply","Fazė","","","","3~","3~","3~"]
["","Dažnis","","","Hz","50","50","50"]
["","Pavadinimas","","","","W1","W1","W1"]
["","Įtampa","","","V","400","400","400"]
["Pastabos","","","","","(1) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(1) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB","(1) - Vėsinimas: EW 12 °C; LW 7 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(2) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(2) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB","(2) - Vėsinimas: EW 23 °C; LW 18 °C; aplinkos sąlygos: 35 °C DB"]
["","","","","","(3) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(3) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(4) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(4) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)","(4) - Sąlyga: Ta DB/WB 7 °C/6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(5) - Pagal EN14825","(5) - Pagal EN14825","(5) - Pagal EN14825"]
["","","","","","(6) - Priklauso nuo darbinio režimo, žr. įrengimo vadovą.","(6) - Priklauso nuo darbinio režimo, žr. įrengimo vadovą.","(6) - Priklauso nuo darbinio režimo, žr. įrengimo vadovą."]
["","","","","","(7) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(7) - Daugiau informacijos rasite veikimo diapazono brėžinyje","(7) - Daugiau informacijos rasite veikimo diapazono brėžinyje"]